# Intel® PRO/100 Adapter Specifications

Product Feature | PRO/100+ Management Adapter | PRO/100 VE Desktop Adapters and Network Connections | PRO/100+ Server Adapter | PRO/100+ Dual Port Server Adapter | PRO/100 S Server Adapter
Bus Connector | PCI 2.2 | CNR 1.0 | PCI 2.2 | PCI 2.2 | PCI 2.2
Transmission Mode/Connector | Twisted copper/RJ-45 | Twisted copper/RJ-45 | Twisted copper/RJ-45 | Twisted copper/RJ-45 | Twisted copper/RJ-45
Cabling | 10BASE-T (Category 3, 4, or 5) 100BASE-TX (Category 5) | 10BASE-T (Category 3, 4, or 5) 100BASE-TX (Category 5) | 10BASE-T (Category 3, 4, or 5) 100BASE-TX (Category 5) | 10BASE-T (Category 3, 4, or 5) 100BASE-TX (Category 5) | 10BASE-T (Category 3, 4, or 5) 100BASE-TX (Category 5)
Power requirements | 0.67 Watts @ 5.0VDC | 0.3 Watts @ 3.3VDC | 0.67 Watts @ 5.0VDC | 6.5 Watts @ +5VDC (715191-00x and 751110-00x) | 1.73 Watts @ 5.0VDC
Operating temperature | 0 - 55 degrees C | 0 - 55 degrees C | 0 - 55 degrees C | 0 - 55 degrees C | 0 - 55 degrees C
Interrupt | INTA | INTA | INTA | INTA | INTA
MTBF | 160 years | 290 years | 160 years | 160 years | 158 years
Available Speeds | 10/100 auto-negotiate | 10/100 auto-negotiate | 10/100 auto-negotiate | 10/100 auto-negotiate | 10/100 auto-negotiate
Duplex modes | Full or half at 10 or 100 Mbps | Full or half at 10 or 100 Mbps | Full or half at 10 or 100 Mbps | Full or half at 10 or 100 Mbps | Full or half at 10 or 100 Mbps
Standards conformance | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x PCI 2.2 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x CNR 1.0 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x PCI 2.2 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x PCI 2.2 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x PCI 2.2
Indicator Lights | Link/Activity 100 TX | Link/Activity 100 TX | Link/Activity 100 TX | (One set per port) Link Activity 100 Mbps | Link/Activity 100 TX
Regulatory and Safety | All adapters: FCC Class B Radiated and Conducted Emissions requirements for U.S. and Canada VCCI Class B Radiated and Conducted Emissions requirements for Japan BSMI Class B Radiated and Conducted Emissions requirements for Taiwan CISPR 22 Class B Radiated and Conducted Emissions requirements for Australia/New Zealand EN55022 Class B Radiated and Conducted Emissions requirements for European Union (EU) EN55024 Immunity requirements for European Union (EU) EN60950 Safety requirements for European Union (EU) UL (Underwriter’s Laboratories) and Canada UL Safety requirements

More adapter information is at the Intel Support web site.

## Standards

- IEEE 802.1p: Priority Queuing (traffic prioritizing) and Quality of Service levels
- IEEE 802.1Q: Virtual LAN identification
- IEEE 802.3u: Fast Ethernet
- IEEE 802.3x: Flow Control
- PCI: system bus specification: 32/64-bit, 33/66 Mhz (any combination, unless otherwise noted)

## Cabling

- 10Base-T on Category 3, 4, or Category 5 wiring, twisted 4-pair copper.
  - Length is 100 meters max.
  - Category 3 wiring supports only 10Mbps.
- 100Base-TX on Category 5 wiring, twisted 4-pair copper.

## Ethernet MAC Addresses

### Single-Port Adapters

The Ethernet address is printed on the identification sticker on the front of the card.

### Integrated Adapters

On a system with the LAN integrated on the motherboard, the identification sticker is usually located on the motherboard near the network connector.

Copyright © 2002 Intel Corporation. Legal Information