==============================================
=  Realtek 8139C/C+ Driver for FreeBSD V4.3  =
==============================================

This driver is modified by Realtek Semiconductor corp. and it has been tested OK
on FreeBSD 4.3. Because the FreeBSD kernel has a default Rtl8139C driver, this 
default driver will be loaded even though the NIC on your computer is Rtl8139C+ 
(because they have the same vender ID and device ID). To use the new features of 
8139C+, you need to update your NIC driver and recompile your FreeBSD kernel.

The main steps you have to do:(FreeBSDSrcDir means the directory of FreeBSD source code
and it may be "/usr/src/sys")

	0.Replace your NIC with 8139C+.
	1.copy if_rl.c and if_rlreg.h to /FreeBSDSrcDir/pci directory
	2.copy rl directory to /FreeBSDSrcDir/modules directory
	3.recompile your kernel	(you must install your FreeBSD source code first !!)

		# cd /usr/src/sys/i386/conf
		# /usr/sbin/config GENERIC
		# cd ../../compile/GENERIC
		# make depend
		# make
		# make install
		# reboot

Q:How to check whether my new driver is working ? 
A:Use the "dmesg|more" command and if you can see "<RealTek 8139C+ 10/100BaseTX>"
  then it is working.

