   LAN Server 4.0

   [1].Introduction:
   -------------
      This document describes the procedure to install NDIS driver on DOS
      LAN Requester and OS/2 LAN server 4.0 for Realtek RTL8139  ethernet
      adapter.

   Location of Driver:  \NDIS2DOS\RTSND.DOS  (for DOS LAN Services)
                        \NDIS2OS2\RTSND.OS2  (for OS/2 LAN Server)

   [2].Installing driver procedure on DOS LAN Requester :
   --------------------------------------------------
      Before you start with the installation  process,  make sure that
      DOS LAN Services is properly installed.  Similarly, your adapter
      should also be properly installed in your client PC.

      1. Copy RTSND.DOS from your Driver diskette (A:\NDIS2DOS)
         to DOS LAN Services subdirectory C:\DLS .

      2. Under DOS LAN Requester subdirectory C:\DLS, run INSTALL

      3. The  screen  display  some description. If it's correct, move
         highlight to "The listed options are correct" item ,then press
         ENTER.

      4. Move highlight to "Network Card", then press ENTER.

      5. Select "Change driver for network card." item, then press ENTER.

      6. Select "Network card not shown in list below..", then press ENTER.

      7. Insert the Realtek RTL8139 driver diskette in floppy A,and specify
         your pathname A:\NDIS2DOS,then press ENTER.

      8. Realtek 8139 driver is now installed on your computer, reboot
         your computer.


   [3].Installing driver procedure on OS/2 LAN Server 4.0:
   ---------------------------------------------------
      Before you start with the installation  process,  make sure that
      OS/2 LAN Server  is properly installed.  Similarly, your adapter
      should also be properly installed in your server.

      1. In OS/2 window, Click the "MPTS" icon.

      2. The screen will display the IBM Log, press "OK".

      3. Select "Install" button.

      4. Insert the REALTEK RTL8139 driver diskette, specify the driver
         path A:\NDIS2OS2 and press <Enter>.

      5. When complete above step to load  RTSND.OS2  into OS/2 system,
         then configure your system.

      6. The same step as step 3, select "Configure" button.

      7. The screen will display "Configure" dialog box and select "LAN
         adapters and protocols" then press "configure" button.

      8. The screen will display "LAPS Configuration" dialog box, move
         highlight to "RTL8139 Fast PCI Ethernet Adapter" item in "Network
         Adapter" window, and select "NetBios"  protocol. Press "OK".

      9. Installation is complete now. Reset your PC by turning it off
          and on.

    [4].Installing Multiple LAN Adapters:
    ----------------------------------
      1.follow [3]. 1-9 and add tow RTL8139 Adapter driver

      2.in IBM Lan Services icon, OS/2 Lan Sercices Installation
                                                           /Configuration
        Select your the server of the insatlled,[OK].
        Do you want to re-install this version.[No].
        Installing tow card driver [OK] in mpts.
        Configure a component. [OK]
        Lan Services Adapters. [OK]
        Configure. [OK]
        Two Adapter [V]. OK


    [5].A sample PROTOCOL.INI file:
    -------------------------------

         [RTL8139]
         DriverName=RTSND$
         EtherID=@52544C111111  ;This  keyword is used to desinate a RTL8139
                                ;adapter by assigning it's ethernet ID
                                ;when more than one adapters exist on one
                                ; system.

         BusNo=@00          ;This  keyword is used to desinate a RTL8139
                            ;adapter by assigning it's PCI bus number
                            ;when more than one adapters exist on one
                            ; system.(must be used with 'DeviceNo' keyword)

         DeviceNo=@0A       ;This  keyword is used to desinate a RTL8139
                            ;adapter by assigning it's PCI Device number
                            ;when more than one adapters exist on one
                            ; system.(must be used with 'BusNo' keyword)

         Medium= 100/10      ;This keyword is used to force RTL8139 adapter
                            ;to speed 10M or 100M mode. If not present,
                            ;the driver will auto-detect the speed.




                                                     -- Jack Chen --

