Broadcom BCM5788 NetXtreme Gigabit Ethernet Drivers INSTALLATION(For Win9x):

1. Open 'Device Manager'.

2. Open the properties for the 'Broadcom Corporation Ethernet controller'.

3. Select 'Update Driver'.

4. Point the installer to the folder with the '\Broadcom\GigaLAN\Win98SE'.

5. It should select the 'b57w9x.inf' and then install the system files.