Back to Contents Page

# Specifications: Broadcom NetXtreme® 57XX User Guide

10/100/1000BASE-T Cable Specifications

Performance Specifications

Environmental Specifications

## 10/100/1000BASE-T Cable Specifications

Port Type | Connector | Media | Maximum Distance
--- | --- | --- | ---
10BASE-T | RJ-45 | Category 3, 4, or 5 unshielded twisted pairs (UTP) | 100m (328 ft)
100/1000BASE-T1 | RJ-45 | Category 52 UTP | 100m (328 ft)
11000BASE-T signaling requires 4 twisted pairs of Category 5 balanced cabling, as specified in ISO/IEC 11801:1995 and ANSI/EIA/TIA-568-A (1995) and tested for additional performance using testing procedures defined in TIA/EIA TSB95. 2Category 5 is the minimum requirement. Category 5e and Category 6 are fully supported.

## Performance Specifications

Feature | Specification
--- | ---
PCI Type Adapters (BCM5702, BCM5705, BCM5705M, BCM5788, BCM5788M)
PCI Data/Address | 32-bit
PCI Data Burst Transfer Rate | 132 MB/s
PCI Modes | Master/Slave
PCI Express Type Adapters (BCM5751, BCM5751M, BCM5789, BCM5789M)
PCI Express Interface | x1 link width
PCI Express Aggregated Bandwidth (transmit and receive) | 625 MB/s (1 lane)
10/100/1000BASE-T | 10/100/1000 Mbit/s (full-duplex)

## Environmental Specifications

Condition | Operating Specification | Storage Specification
--- | --- | ---
Temperature | 0°C to 55°C (+32°F to +131°F) | –40°C to +85°C (–40°F to +185°F)
Relative Humidity | 5% to 85% (noncondensing) 40°C, 16-hr dwells at extremes | 5% to 95% (noncondensing) 10°C/hr
Altitude | Up to 10 000 ft | Up to 35 000 ft
Shock | 10g, 1/2 sine wave, 11 milliseconds | 60g, 1/2 sine wave, 11 milliseconds
Vibration, peak-to-peak displacement | 0.005 in. max (5 Hz to 32 Hz) | 0.1 in. max (5 Hz to 17 Hz)
Vibration, peak acceleration | 0.25g (5 Hz to 500 Hz) (sweep rate = 1 octave/minute) | 0.25g (5 Hz to 500 Hz) (sweep rate = 1 octave/minute)

Back to Contents Page