;DrIvEr DeScRiPtIoN
; VeRsIoN=1.11 Novell LAN Installation Information File for BCM570X.
; CoPyRiGhT=(c) Copyright 2000-2005 Broadcom Corporation. All rights reserved.
; B57.ldi
; Broadcom Corporation

VER:	1.11
SYN:	1.00

DR BCM570X
{

   DES: 	$bcm_1
   HELP:	$bcm_2
   PAR: 	2.00

   FILE: 	B57.LAN

   PROD: 	'PCI.14E4.1644.*.*.*',
   			'PCI.14E4.1645.*.*.*',
   			'PCI.14E4.1646.*.*.*',
   			'PCI.14E4.16A6.*.*.*',
   			'PCI.14E4.1647.*.*.*',
   			'PCI.14E4.16A7.*.*.*',
   			'PCI.14E4.1648.*.*.*',
   			'PCI.14E4.16A8.*.*.*',
   			'PCI.14E4.164d.*.*.*',
   			'PCI.14E4.1653.*.*.*',
   			'PCI.14E4.1654.*.*.*',
   			'PCI.14E4.165d.*.*.*',
   			'PCI.14E4.165e.*.*.*',
   			'PCI.14E4.166d.*.*.*',
   			'PCI.14E4.170d.*.*.*',
   			'PCI.14E4.170e.*.*.*',
   			'PCI.14E4.1696.*.*.*',
   			'PCI.14E4.16c6.*.*.*',
   			'PCI.14E4.16c7.*.*.*',
   			'PCI.14E4.169c.*.*.*',
   			'PCI.14E4.1676.*.*.*',
   			'PCI.14E4.167c.*.*.*',
   			'PCI.14E4.1677.*.*.*',
			'PCI.14E4.1658.*.*.*',
			'PCI.14E4.1659.*.*.*',
            'PCI.14E4.167e.*.*.*',
            'PCI.14E4.169d.*.*.*',
			'PCI.14E4.16dd.*.*.*',
			'PCI.14E4.16f7.*.*.*',
            'PCI.14E4.16fd.*.*.*',
            'PCI.14E4.16fe.*.*.*'




   ;@#	 SPROD:'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@# 			'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@# 			'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter'


   ;@#   CLIENT:B57.LAN
   ;@#	 ALIAS: B57.LAN


   PR	SLOT OPT
   {
	DES:	$bcm_3
	HELP:	$bcm_4
	default: UND
   }

   FR	FrameSelect
   {
	DES:	$bcm_5
	HELP:	$bcm_6

	CD:	$bcm_7
	CH:	'Ethernet_802.2'

	CD:	$bcm_8
	CH:	'Ethernet_802.3'

	CD:	$bcm_9
	CH:	'Ethernet_SNAP'

	CD:	$bcm_10
	CH:	'Ethernet_II'

	Default: 1,2,3,4
   }

   LIST SPEED OPT
   {
		DES: $bcm_11

		HELP: $bcm_12 

		CD: $bcm_13 
		CH: $bcm_14 

		CD: $bcm_15 
		CH: $bcm_16 

		CD: $bcm_17 
		CH: $bcm_18 

		CD: $bcm_19 
		CH: $bcm_20 

		CD: $bcm_21 
		CH: $bcm_22 

		Default: 1

		OutputFormat: 'Speed=%s'
   }

   PR RXBUFFERS OPT
   {
	  DES:  $bcm_23 

	  HELP: $bcm_34 

	  TYPE:    DECIMAL(3)
	  VAL:     2-512

	  Default: 200
	  OutputFormat: 'RxBuffers=%s'
   }

}


DLANG:	4
;English
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."


LANG:	6
;French
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	7
;German
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."


LANG:	8
;Italian
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	14
;Spanish
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	1
;Chinese-Simplified
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	9
;Japanese
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	10
;Korean
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	13
;Russian
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

LANG:	16
;Chinese-Traditional
	$bcm_1 = "NetXtreme Gigabit Ethernet Driver  "
	$bcm_2 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_3 = "Slot Number"
	$bcm_4 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Line Speed"
	$bcm_12 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_13 = "Automatic Detection"
	$bcm_14 = "AUTO"
	$bcm_15 = "100 Mbs Full Duplex"
	$bcm_16 = '100FD'
	$bcm_17 = "100 Mbs Half Duplex"
	$bcm_18 = '100HD'
	$bcm_19 = "10 Mbs Full Duplex"
	$bcm_20 = '10FD'
	$bcm_21 = "10 Mbs Half Duplex"
	$bcm_22 = '10HD'
    $bcm_23 = "Receive Buffers"
    $bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."

