    ©Copyright 2006 Marvell®.
    All rights reserved.

    SetupYukonWin_516E.htm created 05-Dec-2006

    Readme File for SETUPYUKONWIN_516E.exe v9.12.4.3

    Supporting: Marvell Yukon Ethernet Controller

    This package contains the following software components:

    - NDIS5.1 Miniport Driver version 8.61.3.3 for Windows XP/Server 2003 (64 bit)
    - NDIS6 Miniport Driver version 9.12.4.3 for Windows Vista (64 bit)

# This file contains

1 Overview
2 Required File
3 Installation
4 Silent Installation

4.1 Driver Installation
4.2 Driver Removal
4.3 Driver Repair
4.4 Further Options

5 Troubleshooting

## 1 Overview

    The driver installation package contains the Marvell NDIS Miniport Driver
    for the Marvell Yukon Ethernet Controller.

    This README file explains how to install the driver installation package on
    a machine running one of the following operating systems:

    Windows XP/Server 2003 64bit (x64), Windows Vista 64bit

## 2 Required File

    To install the driver, the following file is required:

        SetupYukonWin_516E.exe

## 3 Installation

    On plug & play Windows versions the adapter is found, identified and
    configured automatically. Cancel all operating system attempts to install
    the driver automatically.

    NOTE: To install the driver you have to be logged in as
          a user with administrative rights.

    To install the driver, proceed as follows:

    1. Execute the setup file "SetupYukonWin_516E.exe".
    2. Follow the instructions displayed during the
       installation procedure.

## 4 Silent Installation

    In order to install the driver silently the following commands should be
    executed.

4.1 Driver Installation

    SetupYukonWin_516E.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REBOOT=ReallySuppress /qn"

4.2 Driver Removal

    SetupYukonWin_516E.exe /S /V"/LIME %WINDIR%\YukonInstall.log REMOVE=ALL
    REBOOT=ReallySuppress /qn"

4.3 Driver Repair

    SetupYukonWin_516E.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REINSTALLMODE=vomus REINSTALL=ALL REBOOT=ReallySuppress /qn"

    NOTE: On Windows 98 SE and Windows Me it is recommended
          to use "REBOOT=Force" instead of
          "REBOOT=ReallySupress" because each driver
          installation needs a reboot for completion.

4.4 Further Options

    By default the installation directory is "%PROGRAMFILES%\Marvell\Miniport
    Driver". It can be changed by setting the variable "INSTALLDIR".
    Example :

    SetupYukonWin_516E.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    INSTALLDIR=C:\MyDir REBOOT=ReallySuppress /qn"

    The installation status is logged in the file "%WINDIR%\YukonInstall.log".
    The log file path and name can be changed by replacing
    "%WINDIR%\YukonInstall.log" with the preferred file path and name.

## 5 Troubleshooting

    If you should encounter any problems with your driver installation package,
    please re-read the instructions above and the documentation supplied with
    the operating system carefully.

    Additionally refer to your system event log file (using the Event Viewer)
    and check it for entries from the Marvell NDIS Miniport Driver. If your
    particular problem is not listed or the error persists, please send your
    system event log file to our technical support.

    For further information please contact our support.

    *** End of Readme File ***