; ** COPYRIGHT (C) 2007-2011 Realtek CORPORATION
;
; Realtek PCIe FE Family Controller
; Realtek PCI GBE Family Controller
; Realtek PCIe GBE Family Controller
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
DriverVer   = 03/21/2011,7.043.0321.2011
CatalogFile.NT = rt64win7.cat

[Manufacturer]
%Realtek%=Realtek, NTamd64

[ControlFlags]
ExcludeFromSelect     = *


[Realtek.NTamd64]
; 8169 Cardbus Jumbo 7k
; remeber to remove from OEM INF list 
%R8169C7k.DeviceDesc%  = R8169C7k.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03351154
; 8169 S-32
%SMC9452TX.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_EE221113


; 8169
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&REV_10
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1432&DEV_9230&SUBSYS_92301432
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1432&DEV_9230&SUBSYS_01051432
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1432&DEV_9230&SUBSYS_96041432
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_ED0114EA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_734E1371
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_320210BD
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_310210BD
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_311A1385
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_52001385
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1737&DEV_1032&SUBSYS_00241737
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_16EC&DEV_0116&SUBSYS_011616EC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C1131259
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C1121259
; 8169 OEM IDs
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_102D147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_102F147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1032147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1039147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1045147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105F147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106C147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106D147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106E147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106F147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_180A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2208147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_240A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00361025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006A1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006E1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00711025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00731025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007D1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007E1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007F1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00791025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007D1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009A1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009B1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009F1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201915 ;Acorp
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211915 ;Acorp
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221915 ;Acorp
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231915 ;Acorp
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241915 ;Acorp
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_816917F2 ;Albatron
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_46051961 ;AMOI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F7A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F8A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F9A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03FAA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0405A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0406A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_040CA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_041CA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0449A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_044AA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045BA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045CA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045DA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045EA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045FA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0460A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0461A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0462A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046DA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046EA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0477A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049CA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049DA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049EA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049FA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A0A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A1A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A2A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CAA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CBA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CCA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CDA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0526A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0528A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_052AA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0542A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0543A0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054BA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054DA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054FA0A0 ;Aopen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0563A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0571A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_057CA0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0583A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0589A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058AA0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0600A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0601A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0602A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0604A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_060EA0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_202F161F ;Arima
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10A61043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11E51043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11F51043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81631043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81CB104D ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0121631 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23031565 ;Biostar
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23041565 ;Biostar
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_032B1154 ;Buffalo
;%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03351154 ;Buffalo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F446270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2793270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_272B270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_273B270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F644270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7842270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7860270F ;Chaintech
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_376C1462 ;CHANNEL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00031854 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01201558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02951558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02971558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03751558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04501558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04511558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04521558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04531558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04541558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04701558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04761558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04801558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A01558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05001558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05031558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05041558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05051558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05061558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05071558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05081558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05091558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05201558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05601558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05701558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05711558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05721558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_06601558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07001558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07031558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07041558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08001558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08031558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08041558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08051558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08061558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08071558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08081558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08091558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09001558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09031558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09041558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54051558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001214C0 ;Compal
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001714C0 ;Compal
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_002014CO ;Compal
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3085103C ;Compal
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FF001179 ;Compal
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02B11028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02CB1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02CC1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02CD1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02CE1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A15BD ;DFI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F271019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F471019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F521019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F561019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F661019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F671019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B111019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18651019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18731019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18741019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18531019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18031019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B081019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B101019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81691019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_90221695 ;EPoX
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_28211509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60011509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60021509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60031509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60041509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60051509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60061509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60071509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60081509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60091509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60101509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60111509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60121509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60131509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60141509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60151509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60161509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60171509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60181509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60191509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_601C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_601E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_601F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60251509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60261509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60271509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60281509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60291509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60301509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60311509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60321509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60331509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60341509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60351509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60361509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80011509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80021509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80031509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80041509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80051509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80061509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80071509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80081509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80091509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80101509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80111509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80121509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80131509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80141509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80151509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80161509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80171509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80181509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80191509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80201509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80211509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80221509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80231509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80241509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80251509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80261509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80271509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80281509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80291509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92171509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92181509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_921F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92201509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92221509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92231509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92261509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92451509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92461509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92471509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92481509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92491509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92501509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92511509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92521509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92551509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92561509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92591509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_925A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_925D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92611509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92671509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92691509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92701509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92731509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92741509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92751509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92761509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92771509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92781509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92791509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C06105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C07105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C08105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C09105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C10105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C11105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C12105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C13105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C14105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C15105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C16105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C17105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C18105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C19105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C20105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C21105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C22105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C23105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C24105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C25105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C26105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C27105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C28105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C29105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C30105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C31105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C32105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C33105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C34105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C35105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C36105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C37105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C38105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C39105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C41105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C42105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C43105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C44105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C45105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C46105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C47105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C48105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C49105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C51105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C52105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C53105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C54105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C55105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C56105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C57105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C58105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C59105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C60105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C61105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C62105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C63105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C64105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C65105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C69105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C70105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C71105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C72105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C73105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C74105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C75105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C80105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C81105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C82105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C83105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C84105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C85105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C8E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C90105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C91105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C92105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C93105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C94105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C95105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C97105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C98105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C99105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10911734 ;FSC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10931734 ;FSC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FE001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FE011458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_66661458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_32001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0091631 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_70031631 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0001940 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03001014 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2A17103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_301F103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3022103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3023103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3081103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308F103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3091103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3633103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00071170 ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000A1170 ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000B1170 ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00201170 ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500417FF ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500517FF ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500617FF ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500D17FF ;Inventec
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10EC16F3 ;Jetway
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_811016F3 ;Jetway
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_383617AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3BE617AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80061854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80071854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80081854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80091854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800A1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800B1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800C1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800D1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800E1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800F1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_011616EC ;Liteon_USR
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01241071 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01711071 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80171071 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80501071 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_83171071 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80661071 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0081631 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00A1631 ;Mitac
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003C1462 ;MS-7003
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006C1462 ;MS-7006
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_008C1462 ;MS-7008
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01611462 ;MS-1016
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01611462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02411462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_028C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_033C1462 ;MS-7033
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058C1462 ;MS-7058
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_062C1462 ;MS-7062
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_094C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_097C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_101C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_108C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11501462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_131C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_133C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_139C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_140C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_143C1462 ;MS-7143
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_151C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_166C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_173C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_176C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_177C1462 ;MS-7177
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_183C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_191C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_194C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_19601462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_197C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_204C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_208C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_209C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_210C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_211C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_215C1462 ;MS-7215
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_222C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_223C1462 ;MS-7223
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_229C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_232C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_235C1462 ;MS-7235
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_236C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_240C1462 ;MS-7240
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_241C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_242C1462 ;MS-7242
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_248C1462 ;MS-7248
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_251C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_254C1462 ;MS-7254
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_258C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_267C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_275C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_279C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_327C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_702C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_70941462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_72111462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_728C1462 ;MS-6728
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_758C1462 ;MS-6758
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_76081462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_771C1462 ;MS-6771
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_788C1462 ;MS-6788
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_799C1462 ;MS-6799
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D0071631 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D0081631 ;MS-7168
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E00F1631 ;MS-7069
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0111631 ;MS-7069
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_826E1033 ;NEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_82971033 ;NEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_82B61033 ;NEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_88461033 ;NEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E00F1631 ;NECCI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_833810F7 ;Panasonic
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0746152D ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0729152D ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0730152D ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058A17FF ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058B17FF ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107D1734 ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00B1631 ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00D1631 ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0111631 ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0181631 ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100817AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A17AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3BE617AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_31558452 ;Topstar
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_5003148C ;TUL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020B14FF ;Twinhead
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E14FF ;Twinhead
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020F14FF ;Twinhead
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_021214FF ;Twinhead
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107C1734 ;Uniwill_FjSi
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10AC1734 ;Uniwill_FjSi
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10B01734 ;Uniwill_FjSi
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_51081584 ;Uniwill
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_97101584 ;Uniwill
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003317C0 ;Wistron
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105317C0 ;Wistron
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10921734 ;Wistron
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_109417C0 ;Wistron
%DLINKDGE528T.DeviceDesc%   = RTL8169.ndi, PCI\VEN_1186&DEV_4300&SUBSYS_43001186
%DLINKDGE660TD.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_43011186
%SITECOM.DeviceDesc%        = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0030182D
%ZYXELGN680T.DeviceDesc%    = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_330B187E
%IODATAETGPCI.DeviceDesc%   = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D01F10FC
%IODATAETGCB.DeviceDesc%    = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D03E10FC


; 8168
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
; 8168B OEM IDs
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1071147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1072147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1073147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1074147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1077147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1078147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1079147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107A147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_180F147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_240D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2410147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2412147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01071025&REV_01 ;acer
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_010C1025&REV_01 ;acer
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_26511025&REV_01 ;acer
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0B105B&REV_01 ;acer
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B1331897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B2201897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_060DA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0611A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0614A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0616A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0618A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_061BA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_061CA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0623A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0624A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0625A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0631A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0634A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0636A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_063DA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0640A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0642A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2055161F&REV_01 ;Arima
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_206A161F&REV_01 ;Arima
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_206B161F&REV_01 ;Arima
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11F51043&REV_01 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043&REV_01 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_058D17FF&REV_01 ;BENQ
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_01 ;CHANNEL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462&REV_01 ;CHANNEL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462&REV_01 ;CHANNEL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_369C1462&REV_01 ;CHANNEL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_387C1462&REV_01 ;CHANNEL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E0001940&REV_01 ;Channel
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05211558&REV_01 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05741558&REV_01 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05911558&REV_01 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09021558&REV_01 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_54091558&REV_01 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_002014C0&REV_01 ;Compal
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_002114C0&REV_01 ;Compal
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_002C14C0&REV_01 ;Compal
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;Compal
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02B11028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CB1028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CC1028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CD1028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CE1028&REV_01 ;DELL
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F711019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F721019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F761019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F771019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F811019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F821019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90A21019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_97501019&REV_01 ;ECS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90361695&REV_01 ;Epox
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_601F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60251509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60291509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60301509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60311509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60321509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60331509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60341509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60351509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60361509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60371509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60381509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60391509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603B1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60401509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_801A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_801C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_801D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_801E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_801F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80201509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80211509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80221509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80231509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80241509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80251509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80261509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80271509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80281509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80291509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802B1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C7B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C7C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C7D105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C7E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C88105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C89105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C90105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C91105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0C92105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D0E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D16105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D47105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D4C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DEA105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DEE105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DEF105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF6105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DFD105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0D105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E17105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E18105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E19105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_111C1734&REV_01 ;FSC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11231734&REV_01 ;FSC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11241734&REV_01 ;FSC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_01 ;FSC(D45/D46)
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B&REV_01 ;GATEWAY
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_01 ;Gigabyte
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30B6103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30CC103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00401170&REV_01 ;Inventec
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_500E17FF&REV_01 ;Inventec
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6068086&REV_01 ;Intel
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6088086&REV_01 ;Intel
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816816F3&REV_01 ;JETWAY
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_01 ;LGE
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_01 ;LGE
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_01 ;LGE
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_01 ;LGE
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_104D13BD&REV_01 ;MiTAC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_47001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_47011071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01111462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01211462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01311462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01611462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02211462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02411462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02911462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03211462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03411462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_034A1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03611462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03911462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03711462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_040D1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04711462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05311462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05711462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106F1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_238C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_270C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_276C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_280C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2F8B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2FB11462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2FB31462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2FBD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_309C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_327C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_33201462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_33371462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_337C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_33411462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_334B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_34131462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_359C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_368C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373D1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_379C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_395C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3EF91462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3F711462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FB91462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FCC1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FD51462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FDF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FF41462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3FFE1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_42CD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_42D71462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_42E11462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43101462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43141462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43241462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43271462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_502C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_514C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_63701462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_63F21462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_63F41462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_64701462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65301462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_71901462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_71F11462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_72101462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_72301462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_732A1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_732B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4121462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4221462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_303017AA&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80111854&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80161854&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80171854&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2F811462&REV_01 ;MSI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_18548011&REV_01 ;MSI_SI
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83841033&REV_01 ;NEC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033&REV_01 ;NEC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631&REV_01 ;NEC
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20021B0A&REV_01 ;PEGATRON
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_056017FF&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_058F17FF&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0761152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0762152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0763152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B052144D&REV_01 ;SAMSUNG
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B057144D&REV_01 ;SAMSUNG
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00051290&REV_01 ;TOPS
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_01 ;TOSHIBA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_01 ;TOSHIBA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF101179&REV_01 ;TOSHIBA
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10CD1734&REV_01 ;Uniwill(FSC)
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11071734&REV_01 ;Uniwill(FSC)
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90761584&REV_01 ;Uniwill
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10C317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A00D14FF&REV_01 ;XPLORE

; 8112
%RTL8112.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83851043&REV_01


; 8101
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
; 8101E OEM IDs
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_180E147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_180F147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_240F147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_010C1025&REV_01 ;ACER
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02451025&REV_01 ;ACER
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_026C1025&REV_01 ;ACER
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_26721025&REV_01 ;ACER
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_B10A1897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_BD891897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_BC891897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0618A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_063DA0A0&REV_01 ;AOPEN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2055161F&REV_01 ;Arima
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_206A161F&REV_01 ;ARIMA
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_206B161F&REV_01 ;ARIMA
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_12F51043&REV_01 ;ASUS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_12F61043&REV_01 ;ASUS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_81361043&REV_01
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C10A1631&REV_01 ;ASUS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2101631&REV_01 ;ASUS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2121631&REV_01 ;ASUS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E0381631&REV_01
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_302C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_313C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_376C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_387C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_525C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_528C1462&REV_01 ;CHANNEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_529C1462&REV_01
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E0001940&REV_01 ;Channel
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_06211558&REV_01 ;CLEVO
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_027D1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_027E1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02AD1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B11028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B41028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CB1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CC1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CD1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CE1028&REV_01 ;DELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0F961019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2B301019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_81361019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90A01019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90A11019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90A21019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90AC1019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B11019&REV_01 ;ECS
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90371695&REV_01 ;Epox
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_601F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60251509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60291509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60301509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60311509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60321509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60331509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60341509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60351509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60361509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60371509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60381509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60391509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60401509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60411509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60421509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60431509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60441509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60451509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60461509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60471509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60481509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_604A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_604B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_604C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_604D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_604E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_801A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_801C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_801D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_801B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_801E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_801F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80201509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80211509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80221509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80231509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80241509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80251509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80261509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80271509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80281509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80291509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_802A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_802B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_802C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_802D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_802E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_802F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0C76105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0CE6105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0CF7105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D1B105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D1C105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D40105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D41105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D42105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D47105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D48105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D4A105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D4B105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D4F105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DD6105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DDA105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DE2105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DE3105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DE9105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DEA105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DED105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DEE105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DF6105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DF7105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E0C105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E0D105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E19105B&REV_01 ;FOXCONN
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11071734&REV_01 ;FSC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11081734&REV_01 ;FSC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_110A1734&REV_01 ;FSC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11231734&REV_01 ;FSC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_01 ;FSC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_01 ;FSC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0368107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0560107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0561107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0565107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0566107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30BA103C&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30CC103C&REV_01
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0380107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0381107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0386107B&REV_01 ;Gateway
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_301A17AA&REV_01 ;GIGABYTE
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10128086&REV_01 ;INTEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_D6078086&REV_01 ;INTEL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00161170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00371170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00411170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813616F3&REV_01 ;JETWAY
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_01151854&REV_01 ;LGE
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_01161854&REV_01 ;LGE
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_20001854&REV_01 ;LGE
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_20011854&REV_01 ;LGE
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_104D13BD&REV_01 ;MiTAC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_276C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_314C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_327C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_337C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_359C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_368C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_373C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_379C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3FBB1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_43401462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_44101462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_502C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_536C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_63F11462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_63F61462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_66101462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_732A1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_732B1462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_75261462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_75291462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_75351462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_75651462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_75691462&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_303017AA&REV_01 ;MSI
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10271631&REV_01 ;NEC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C0271631&REV_01 ;NEC
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C10C1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C10D1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E0311631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E03B1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_01991025&REV_01 ;PEGATRON
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_200C1B0A&REV_01 ;PEGATRON
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_B05F144D&REV_01 ;SAMSUNG
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105213BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105313BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105413BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_9015104D&REV_01 ;SONY
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00011179&REV_01 ;TOSHIBA
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_01 ;TOSHIBA
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179&REV_01 ;TOSHIBA
;%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;TOSHIBA
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF501179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2B301584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_97001584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_01 ;WHITE BOX
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2161631&REV_01 ;Wistron
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_01 ;Wistron
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_01 ;Wistron
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_23061565&REV_01

; 8131
%RTL8131.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83A01043&REV_01

; 8101HP
%RTL8136HP.DeviceDesc%  = RTL8136HP.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A89103C ;HP
%RTL8136HP.DeviceDesc%  = RTL8136HP.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30CB103C ;HP
%RTL8136HP.DeviceDesc%  = RTL8136HP.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

; 8136HP S5 WOL Default Disable 
%RTL8136HP.DeviceDesc%  = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A60103C ;HP
%RTL8136HP.DeviceDesc%  = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136HP.DeviceDesc%  = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136HP.DeviceDesc%  = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A59103C ;HP
%RTL8136HP.DeviceDesc%  = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136HP.DeviceDesc%  = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A7B103C ;HP


; 8167
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_816710EC
; 8167 OEM IDs
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_009A1025 ;Acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_009B1025 ;Acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_009F1025 ;Acer
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1077147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_107B147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_107D147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_107E147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1080147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1082147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1083147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1087147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1088147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_108A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_108B147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_108D147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1423147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1424147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1425147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_180A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1C2A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_240B147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_240C147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_240E147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_13451043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_820D1043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_376C1462 ;CHANNEL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_76341462 ;OEM_Fujitsu
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02951558 ;CLEVO
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02961558 ;CLEVO
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_05711558 ;CLEVO
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_06601558 ;CLEVO
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_07201558 ;CLEVO
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_54051558 ;CLEVO
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02B11028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02CB1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02CC1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02CD1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_02CE1028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_05091028 ;DELL
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_81671019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_81691019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_90381695 ;Epox
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60041509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60081509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_601C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_601D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_601E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_601F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60211509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60221509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60231509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60241509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60251509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60271509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60291509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_602A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_602B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_602C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_602D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60301509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60311509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60321509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60331509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60341509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60351509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60361509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60371509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60381509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60391509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_603A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_603B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_603C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_603D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_603E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_603F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60401509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60411509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60421509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60431509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60441509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60451509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60461509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60471509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60481509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_60491509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_604A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_604B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_604C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_604D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_604E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_604F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80021509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_801A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_801B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80201509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80211509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80221509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80231509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80241509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80251509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80261509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80271509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80281509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80291509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_802A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_802B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_802C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_802D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_802E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_802F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C06105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C07105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C08105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C09105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C0A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C0B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C0C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C0D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C0E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C0F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C10105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C11105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C12105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C13105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C14105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C15105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C16105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C17105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C18105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C19105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C1A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C1B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C1C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C1D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C1E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C1F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C20105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C21105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C22105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C23105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C24105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C25105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C26105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C27105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C28105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C29105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C2A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C2B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C2C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C2D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C2E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C2F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C30105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C31105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C32105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C33105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C34105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C35105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C36105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C37105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C38105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C39105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C3A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C3B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C3C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C3D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C3E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C3F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C41105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C42105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C43105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C44105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C45105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C46105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C47105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C48105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C49105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C4A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C4B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C4C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C4D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C4E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C4F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C51105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C52105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C53105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C54105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C55105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C56105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C57105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C58105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C59105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C5A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C5B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C5C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C5D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C5E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C5F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C61105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C62105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C63105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C64105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C65105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C66105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C67105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C68105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C69105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C6B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C6C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C6D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C6E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C6F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C70105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C71105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C72105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C73105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C74105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C79105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C7B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C7C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C7D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C7E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C80105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C81105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C82105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C83105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C84105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C85105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C86105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C87105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C88105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C89105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C8D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C90105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C91105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C92105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C93105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C94105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C95105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C96105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C97105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C98105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C99105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C9A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C9B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C9C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C9D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C9E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0C9F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CA8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CAA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CAB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CAC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CAD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CAE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CAF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CC5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CC6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CC7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CC8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CC9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CCA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CCB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CCC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CCD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CCE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CCF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CE8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CE9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CEA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CEB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CF8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CFA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CFB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CFC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CFD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CFE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0CFF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D09105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D0C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D19105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D1A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D1F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D45105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D46105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0D75105B ;Foxconn_Clone
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0DE5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0DF9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0E0E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0E10105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_0E13105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_10D01734 ;FSC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_302A103C ;Gigabyte
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_E0001458 ;Gigabyte
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_302A103C ;Gigabyte
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_2A37103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_3022103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_3023103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_3024103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_3028103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_3633103C ;HP
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_06101170 ;INVENTEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_07101170 ;INVENTEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_100717AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_100A17AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_383617AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_383A17AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_800D1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_80101854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_800D1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_197C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_251C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_258C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_263C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_277C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_279C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_280C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_281C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_280C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_300C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_305C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_312C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_318C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_33101462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_332C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_333C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_376C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_381C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_70941462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_76081462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_76341462 ;MSI_Fujitsu
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_18548012 ;MSI_SI
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_A0231071 ;MITAC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_88031033 ;NEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_88461033 ;NEC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_C0191631 ;RT_QTA
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_30941297 ;Shuttle
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1100147B ;UABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_1107147B ;UABIT
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_008317C0 ;Wistron


; 8168C
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
; 8168C OEM IDs
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B2301897&REV_02 ;AMTEK
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13601019&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01361025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_013E1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01401025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01441025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_014C1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_016D1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_016E1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02291025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02381025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_025F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02611025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_026F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_027F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02801025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02811025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02821025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02831025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02841025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02851025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02861025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02871025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02881025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02891025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_028A1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_028B1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03021025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03031025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03041025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03291025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_032A1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_032B1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_063AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0640A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0642A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0643A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0644A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0646A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0648A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_064AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_064BA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_064EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0700A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0703A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_234EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03E91AA7&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_02 ;ASUS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C61043&REV_02 ;ASUS
; Please note : 82FF1043, 83AB1043 use a specific inf entry
;%RTL8168C.DeviceDesc% = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS
;%RTL8168C.DeviceDesc% = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02 ;ASUS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C2111631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C2131631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080117FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080217FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080317FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080517FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_090017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0772152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0773152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0774152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0775152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0776152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0779152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0780152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0817152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0823152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1777152D&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_398C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_501C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_513C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_519C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_528C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_73751462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75301462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75331462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75501462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75511462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01221558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01261558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03901558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04811558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07221558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_072F1558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08051558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08061558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08601558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09031558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_56011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_70011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76401558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76411558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_016B107B&REV_02 ;COMPAL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_016D107B&REV_02 ;COMPAL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02581028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_026F1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02731028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02751028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02791028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_027D1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_027E1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02821028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02831028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02851028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02A91028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02AC1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02B11028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02B51028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CB1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CC1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CD1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02CE1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02D91028&REV_02 ;DELL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81111019&REV_02 ;ECS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_02 ;ECS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AD1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50011509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50021509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50031509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50041509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50051509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60331509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60341509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60351509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60361509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60371509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60381509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60391509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603D1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603E1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_603F1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60401509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80201509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80211509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80221509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80281509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80291509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D16105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D4C105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DDB105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE7105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DE9105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DEA105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DEE105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DEF105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF0105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DFD105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E17105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E18105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E19105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E1C105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11231734&REV_02 ;FSC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11241734&REV_02 ;FSC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11351734&REV_02 ;FSC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B&REV_02 ;GATEWAY
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0900107B&REV_02 ;GATEWAY
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_000E1B0A&REV_02 ;HAIER
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_001F1B0A&REV_02 ;HAIER(EPSON)
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1505103C&REV_02 ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1506103C&REV_02 ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A73103C&REV_02 ;HP bPC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A80103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A88103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2B00103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2B10103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2B22103C&REV_02 ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2B23103C&REV_02 ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3038103C ;HP-CDC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_303A103C ;HP_pinatubo
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_303B103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3043103C ;HP_nujiang
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3045103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3046103C ;HP_huangpu
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30DE103C ;HP(INVENTEC)
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30F1103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30F2103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30F4103C ;HPQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30F8103C ;HPQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30FB103C ;HPQ
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30FC103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3600103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3602103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3603103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_360F103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3610103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_361B103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_361C103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_361D103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_361E103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3621103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3622103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3623103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3624103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3627103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3628103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3629103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3633103C ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7010103C&REV_02 ;HP
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_434E8086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6098086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6128086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6218086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_011F1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01201854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01211854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01221854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20021854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20031854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20071854&REV_02 ;LGE
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17741854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17751854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17761854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17791854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17801854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17881854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17891854&REV_02 ;LG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10051462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10081462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10181462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103F1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10401462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_22701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_365C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_395C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43501462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_43801462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_515C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_520C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_522C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_536C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_63F51462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67401462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_71F01462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_72101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_72201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_72301462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_73881462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75121462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75161462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75221462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75261462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75321462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75351462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75431462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75461462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75491462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75521462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75581462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75641462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75661462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75691462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75721462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75931462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A1101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83691033&REV_02 ;NEC
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00031B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_006A1B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_200B1B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0777152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B04E144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B052144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B057144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B063144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00201B0A&REV_02 ;SI
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60301509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60311509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60321509&REV_02 ;STD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82E919DB&REV_02 ;TCL
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_02 ;THINKPAD
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00091290&REV_02 ;TOPS
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60341991&REV_02 ;TOPSTAR
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00011179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF1F1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF671179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF7A1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_109C147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1102147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1103147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003014C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003114C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003214C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003314C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003414C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003514C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003614C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003714C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003914C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003C14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003D14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_003E14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A00C14FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A01514FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A01614FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A02014FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11631734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10C017C0&REV_02 ;WISTRON(M08B1)
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_409017C0&REV_02 ;WISTRON(MAKI2)

; HP 8168C S5 WOL Default Disable
%RTL8168C.DeviceDesc%  = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A6F103C&REV_02;HP cPC
%RTL8168C.DeviceDesc%  = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A74103C;HP
%RTL8168C.DeviceDesc%  = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A7F103C;HP
%RTL8168C.DeviceDesc%  = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A82103C;HP
%RTL8168C.DeviceDesc%  = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A85103C;HP
%RTL8168C.DeviceDesc%  = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A8A103C;HP

; 8168C_NotSpdDown
%RTL8168C.DeviceDesc%  = RTL8168CNotSpdDown.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02

; 8168C_Force_Gigabit
%RTL8168C.DeviceDesc%  = RTL8168CForceGigabit.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02

; 8168CP_Force_100_Full
%RTL8136.DeviceDesc%  = RTL8168CForce100Full.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2100146C&REV_02


; 8102E
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_015A1025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_015B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_017B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_019B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02441025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02451025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02551025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02561025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_025A1025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02661025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02671025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02761025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_028C1025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02971025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_03011025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80001025&REV_02 ;ACER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_064BA0A0&REV_02 ;AOPEN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0300196F&REV_02 ;AVG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_059817FF&REV_02 ;BENQ
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_059917FF&REV_02 ;BENQ
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_059A17FF&REV_02 ;BENQ
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_059B17FF&REV_02 ;BENQ
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_059C17FF&REV_02 ;BENQ
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_01301558&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08901558&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_71201558&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0772152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0773152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0774152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0775152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0776152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0779152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0780152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0817152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1777152D&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_70011558&REV_02 ;CLEVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86891558&REV_02 ;CLEVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0184107B&REV_02 ;COMPAL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02741028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02971028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02981028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02991028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_029A1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02A91028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02AD1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B01028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B11028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B21028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B41028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B51028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02B81028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02C61028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CB1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CC1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CD1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CE1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02CF1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02D81028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02DF1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02E01028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02E11028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02E21028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02F41028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_02FA1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04011028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04021028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04031028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_040E1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04131028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04151028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04161028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04171028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_041A1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_041E1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_041F1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_042C1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_042E1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_042F1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04341028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04351028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04361028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04471028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04481028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04511028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04521028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04531028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04541028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04591028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_045C1028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04721028&REV_02 ;DELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_237A1019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_81021019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_81031019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_82481019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83481019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90871019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90891019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90921019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B31019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B41019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90931019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90941019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90951019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90961019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B51019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B61019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B71019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90B91019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90BA1019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C01019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C31019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C41019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C51019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C61019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C71019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_90C91019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99701019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99741019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99771019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99B51019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99C71019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99CA1019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99D01019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_A1001019&REV_02 ;ECS
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50011509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50021509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50031509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50041509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50051509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50061509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50071509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50081509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50091509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50101509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50111509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50121509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50131509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50141509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50151509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50161509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50171509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50181509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50191509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50201509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50211509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50221509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50231509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50241509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50251509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50261509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50271509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50281509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50291509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50301509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50501509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60331509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60341509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60361509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60381509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60391509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60411509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60441509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60451509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60461509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60471509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60481509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60501509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80201509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80211509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80221509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80231509&REV_02 ;FIC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0CF7105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D4B105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D76105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DC0105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DC1105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DD6105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DDA105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DE9105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DEA105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DED105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DEE105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DF6105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0DF7105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E19105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E25105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_02 ;FSC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_02 ;FSC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11601734&REV_02 ;FSC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_11611734&REV_02 ;FSC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_118D1734&REV_02 ;FSC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_118E1734&REV_02 ;FSC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_153110CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_153410CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_153510CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_40021B0A&REV_02 ;HAIER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_40091B0A&REV_02 ;HAIER
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0336103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_046B103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1602103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1604103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1605103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1606103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1607103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_162E103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A88103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3054103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3055103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3059103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3060103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3061103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3062103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3063103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3064103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3069103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_306A103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_306B103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_306C103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_306D103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30DE103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30F2103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30F3103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30F4103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30F7103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30FB103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30FC103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30FE103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3600103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3602103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3603103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3607103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_360B103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3621103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3622103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3623103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3624103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3627103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3628103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3629103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3635103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3636103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3637103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3638103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3639103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363A103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363B103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363C103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363D103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363E103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363F103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3642103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3643103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3644103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3649103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3650103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3652103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3656103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3657103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3658103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3659103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_365C103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3660103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3661103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3662103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3663103C ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_7010103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10128086&REV_02 ;INTEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_42498086&REV_02 ;INTEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_D6228086&REV_02 ;INTEL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00051170&REV_02 ;INVENTEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_213117AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_219D17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_21C717AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_21C817AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_21C917AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_21CA17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_300E17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_300F17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_306717AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_360117AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_360617AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_389E17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_392617AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_392E17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_07991854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08001854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08051854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08241854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08251854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08261854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08271854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08281854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08421854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08431854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08441854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08451854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08461854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08471854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08481854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08491854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17721854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17731854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17741854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17751854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17761854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17791854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17801854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17811854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17821854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17831854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17841854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17851854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17861854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17871854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17881854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17891854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_17901854&REV_02 ;LG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00021B7D&REV_02 ;MALATA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_92101071&REV_02 ;MITAC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_A0291071&REV_02 ;MITAC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_74001057&REV_02 ;MOTOROLA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_01101462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_100A1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10171462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_101E1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10271462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10281462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_102B1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10311462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10331462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10381462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10391462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_103C1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_104E1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_104F1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_106B1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_108F1462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10981462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_67201462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_76301462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_76361462&REV_02 ;MSI
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_88FA1033&REV_02 ;NEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_890F1033&REV_02 ;NEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_89311033&REV_02 ;NEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_89421033&REV_02 ;NEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_89511033&REV_02 ;NEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_89621033&REV_02 ;NEC
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_018B1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_018C1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_01931631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2141631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2151631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E2161631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E2171631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_E21B1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_201F1B0A&REV_02 ;PEGATRON
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_20341B0A&REV_02 ;PEGATRON
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0777152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0778152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0781152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0782152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0783152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0784152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0785152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0786152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0787152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0788152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0789152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0792152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0859152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0860152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_B05F144D&REV_02 ;SAMSUNG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_B065144D&REV_02 ;SAMSUNG
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105713BD&REV_02 ;SHARP
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602A1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602B1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602C1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602D1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602E1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_602F1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60301509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60311509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60321509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60351509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60371509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603A1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603B1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603C1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603D1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603E1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_603F1509&REV_02 ;STD
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60301991&REV_02 ;TOPSTAR
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00021179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00031179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD791179&REV_02 ;TOSHIBA
;%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF1F1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF301179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF401179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF641179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF661179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF671179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF681179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF6A1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FFC01179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003014C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003114C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003214C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003314C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003414C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003514C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003614C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003714C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003C14C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003D14C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003E14C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_004614C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_004814C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_004914C0&REV_02 ;WB
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_02 ;WHITE BOX
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_C2161631&REV_02 ;WISTRON
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_02 ;WISTRON
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_02 ;WISTRON
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10C617C0&REV_02 ;WISTRON
%RTL8102.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_112317C0&REV_02 ;WISTRON

; HP 8102E S5 WOL Default Disable
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A85103C ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A8A103C ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A8C103C ;HP_eton
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A97103C ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A98103C ;HP_elvas
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A9D103C ;HP_evans
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A9F103C ;HP_fiano
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA3103C ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA4103C ;HP_edwards
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB0103C ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB8103C ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB9103C ;HP

; HP 8102E S5 WOL Hide and Default Enable
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1414103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1425103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1426103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1427103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1428103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1429103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_142A103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1430103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1431103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1439103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143A103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143B103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143C103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143F103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1440103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1441103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1442103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1443103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1444103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1445103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1446103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1447103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1448103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1449103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144A103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144B103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144C103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144D103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1469103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_146A103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_146B103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_146C103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1474103C&REV_02 ;HP_Valima
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1475103C&REV_02 ;HP_Valima
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1476103C&REV_02 ;HP_Villemont
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_147B103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_147C103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1484103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1485103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_148B103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_149C103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_149D103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_149E103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1526103C&REV_02 ;HP_Villemont
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1580103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1581103C&REV_02 ;HP
%RTL8102.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1582103C&REV_02 ;HP

;;Compal 8103EL Force Enable Clock Request
%RTL8102.DeviceDesc%  = RTL8102ForceEnableClkReq.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_02 ;TOSHIBA


; 8168D
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_019B1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_024E1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_024F1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_025A1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02661025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02671025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02751025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02761025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02971025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_26511025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_038E1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03901025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_039A1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80001025&REV_03 ;ACER
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A1831B72&REV_03 ;AOC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A2161B72&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0700A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0706A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0707A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0708A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0709A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070AA0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070BA0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070CA0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070DA0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070FA0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03E91AA7&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14011849&REV_03 ;ASROCK
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_03 ;ASUS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080417FF&REV_03 ;BENQ
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01261558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01301558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_56011558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86871558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86891558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02BA1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02BB1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02BC1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02BD1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02C01028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02D81028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02EA1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02EB1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02F21028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02F51028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04011028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04021028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04031028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04081028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04131028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04151028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04161028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04171028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04181028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_041B1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_041E1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_041F1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_042B1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04341028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04351028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04391028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_043F1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04401028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04411028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04421028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_045C1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04831028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04E81028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04E91028&REV_03 ;DELL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_237A1019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_811D1019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8D481019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90931019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90B61019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90B71019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90C31019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90C41019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90C51019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90C61019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90C71019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99741019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99771019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99C71019&REV_03 ;ECS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50031509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50041509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50051509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50061509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50071509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50081509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50091509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50101509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50111509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50121509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50131509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50141509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50151509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50161509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50171509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50251509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50501509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60501509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80221509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80231509&REV_03 ;FIC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D47105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D73105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DBF105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC0105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC1105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC6105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC7105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC9105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DCA105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DD4105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF6105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DF7105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0C105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E0D105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E25105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E36105B&REV_03 ;FOXCONN_Clone
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11601734&REV_03 ;FSC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11611734&REV_03 ;FSC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_118D1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_118E1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_153110CF&REV_03 ;FUJI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0256103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1600103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1601103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1602103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1603103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_162C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_162D103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_162F103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1639103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_163A103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_163B103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_163C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_163D103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_163E103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_163F103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1640103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1641103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1642103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1643103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1644103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA1103C ;HP_E61_b
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3059103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3060103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3061103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3062103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3063103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3064103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_306D103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30F7103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3635103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3636103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3637103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3638103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3639103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363A103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363B103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363C103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363D103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363E103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363F103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3652103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3658103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3659103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_365C103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3660103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3661103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3662103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3663103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3664103C ;HP_pine
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3665103C ;HP_oak
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3666103C ;HP_birch
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7001103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7010103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00671170&REV_03 ;INVENTEC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00681170&REV_03 ;INVENTEC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00851170&REV_03 ;INVENTEC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_57568086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6138086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6148086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_213117AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21C517AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21C617AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21C717AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21C817AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21C917AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21CA17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21DD17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21DF17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_305A17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_305B17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_306817AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_306917AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_360A17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_360E17AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_361917AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A017AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392617AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07991854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08001854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08051854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08241854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08251854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08261854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08271854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08281854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08421854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08431854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08441854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08451854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08461854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08471854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08481854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08491854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17741854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17751854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17761854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17791854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17801854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17811854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17821854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17831854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17841854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17851854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17861854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17871854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17881854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17891854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17901854&REV_03 ;LG
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00021B7D&REV_03 ;MALATA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_92231071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_92701071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A0361071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A0381071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E1201071&REV_03 ;MITAC_GeTAC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_74001057&REV_03 ;MOTOROLA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10041462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10061462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10081462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100E1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100F1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10111462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10121462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_101C1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_101D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_101F1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10201462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10211462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10221462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102C1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10301462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10331462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10361462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10391462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103A1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103B1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103E1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10411462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10441462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10481462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_104B1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10501462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10521462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10531462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10551462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10591462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105A1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10651462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10921462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_45701462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_501C1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_633A1462&REV_03 ;MSI_OEM
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_74571462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75191462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75261462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75491462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75501462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75511462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75521462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75631462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75741462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75761462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75771462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75791462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75801462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75811462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75831462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75841462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75851462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75861462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75871462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75881462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75891462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75921462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75951462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75961462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_75991462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76021462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76091462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76151462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76161462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76181462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_761A1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76211462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76221462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76331462&REV_03 ;MSI_OEM
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76351462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76361462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76371462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76381462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76391462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76401462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76421462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76461462&REV_03 ;MSI_Medion
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76531462&REV_03 ;MSI_OEM
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76581462&REV_03 ;MSI_OEM
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76601462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76611462&REV_03 ;MSI_Medion
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76661462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76681462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76751462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76861462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76881462&REV_03 ;MSI_CHANNEL
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77081462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A1101462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AC411462&REV_03 ;MSI
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89421033&REV_03 ;NEC
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12021849&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15011849&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00521B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_008D1B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00931B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_009D1B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00B91B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20221B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_203C1B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_400A1B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0784152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0785152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0786152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0787152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0788152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0789152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0792152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105813BD&REV_03 ;SHARP
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00101290&REV_03 ;TOPS
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60321991&REV_03 ;TOPSTAR
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00021179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FD691179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF1F1179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FF401179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FFC01179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A02414FF&REV_03 ;Twinhead
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004614C0&REV_03 ;WB
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004814C0&REV_03 ;WB
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004914C0&REV_03 ;WB
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10CB17C0&REV_03 ;WISTRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10D017C0&REV_03 ;WISTRON
%RTL8168D.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10D117C0&REV_03 ;WISTRON

; HP 8168D S5 WOL Default Disable
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A8E103C ;HP_jesse
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A90103C ;HP_indio
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A92103C ;HP_aloe
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A94103C ;HP_eureka3
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A97103C ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A9C103C ;HP_iona
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA2103C ;HP_boma
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA3103C ;HP_boma-d
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA0103C ;HP_e46
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A9A103C ;HP_e66
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA5103C ;HP_elkhart
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA6103C ;HP_Matadi

; HP 8168D S5 WOL Hide and Default Enable
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1405103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1407103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1409103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1411103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1412103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1413103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1420103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1421103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1423103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1425103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1426103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1427103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1428103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1429103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142A103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142B103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142D103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1430103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1431103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1433103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1434103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1435103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1436103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1437103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_143D103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_143F103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1440103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1441103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1442103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1443103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1448103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1449103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144A103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144B103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144D103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144E103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1469103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146A103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146B103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1474103C&REV_03 ;HP_Valima
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1475103C&REV_03 ;HP_Valima
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1476103C&REV_03 ;HP_Villemont
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147B103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147F103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1482103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1484103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1485103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1486103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1488103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148B103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149B103C&REV_03 ;HP_Fossil2.0
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149C103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1526103C&REV_03 ;HP_Villemont
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1580103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1581103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1582103C&REV_03 ;HP
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1583103C&REV_03 ;HP_Neon1.0
%RTL8168D.DeviceDesc%  = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1590103C&REV_03 ;HP


; 8112L
%RTL8112L.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A31043&REV_03


; 8168DP
%RTL8168DP.DeviceDesc% = RTL8168DP.ndi, PCI\VEN_10EC&DEV_8168&REV_04
%RTL8168DP.DeviceDesc% = RTL8168DP.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_04


; 8168E
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&REV_06
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_06
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_025B1025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_045C1025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_045D1025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_050A1025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_050B1025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05181025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05191025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05491025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_054A1025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05531025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05541025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05641025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05661025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05961025&REV_06 ;Acer
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A2141B72&REV_06 ;AOC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080AA0A0&REV_06 ;Aopen
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100C1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_101C1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102C1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103C1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_104C1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105C1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84321043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849B1043&REV_06 ;ASUS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04371028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04461028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04671028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04681028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_046B1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_046C1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_046D1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_046E1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04771028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04781028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04791028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_047D1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_049C1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04AF1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B01028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B11028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B21028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B31028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B51028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B61028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B71028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04B81028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04BD1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04BE1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04BF1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C01028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C11028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C41028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C51028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C61028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C71028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04C91028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04CA1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04CB1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04CC1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04CD1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D01028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D11028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D41028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D51028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D71028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D81028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04D91028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04DA1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04ED1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04EE1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04EF1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04F01028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04F11028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04F21028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04F31028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04F41028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04F51028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05021028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05031028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05041028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05051028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05061028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05071028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05081028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_050E1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05111028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05121028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05131028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_051C1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_051D1028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05261028&REV_06 ;DELL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_22DA1019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_811E1019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99821019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99CD1019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99D21019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99D41019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99D51019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99D81019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_99DB1019&REV_06 ;ECS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50141509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50151509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50161509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50171509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50181509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50191509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50201509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50211509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50221509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50231509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50241509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50251509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50261509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50271509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50281509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50291509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50301509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50311509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50321509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50331509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50341509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50351509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50361509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50371509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50381509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50391509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50401509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60501509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60511509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60521509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60531509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60541509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60551509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60561509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60571509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60581509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60591509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60601509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_70041509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_70051509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_70061509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_70081509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_70091509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80241509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80251509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80261509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80271509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80281509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80301509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80311509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80321509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80331509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80341509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80351509&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A214160B&REV_06 ;FIC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D70105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D72105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D77105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D78105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D79105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DBD105B&REV_06 ;FOXCONN
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC8105B&REV_06 ;FOXCONN_Channel
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DC9105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DCB105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DCC105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DCD105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DCE105B&REV_06 ;FOXCONN_Channel
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DCF105B&REV_06 ;FOXCONN_Channel
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0DDD105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E26105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E28105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E29105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E37105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E38105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E39105B&REV_06 ;FOXCONN_Clone
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_020010CF&REV_06 ;Fuji
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_311510CF&REV_06 ;Fuji
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_05191024&REV_06 ;Gateway
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10E417C0&REV_06 ;Generic
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_40001071&REV_06 ;Getac
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B3011071&REV_06 ;Getac
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B3021071&REV_06 ;Getac
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1610103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1611103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1613103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1614103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1615103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1616103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1617103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1624103C&REV_06 ;HP_Jiading
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1625103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1646103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1647103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1649103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164A103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164B103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164C103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164D103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164E103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1656103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1657103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1658103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1659103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_165A103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_165B103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1673103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1674103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1688103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1689103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1775103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1776103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAA103C ;HP_Alder
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABD103C ;HP_Kallang
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3388103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3389103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_355B103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_355C103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_355D103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_355E103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_355F103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3560103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3581103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3582103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3583103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_358B103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_358C103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_358D103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_358E103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_358F103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3590103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3591103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3592103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3593103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3667103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_366A103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_366B103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_366C103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3670103C ;HP_Continental
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3672103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3673103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3674103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3675103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_152D8086&REV_06 ;Intel
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21E117AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21E217AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21E417AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21EA17AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_307217AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_307617AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_307A17AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_361417AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_362817AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_362917AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_362A17AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_395817AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_397517AA&REV_06 ;Lenovo
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08931854&REV_06 ;LG
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08941854&REV_06 ;LG
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08951854&REV_06 ;LG
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30001854&REV_06 ;LG
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30011854&REV_06 ;LG
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10631462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10681462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106A1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106C1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106D1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106E1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10701462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10721462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10731462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10751462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10781462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10791462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107D1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107E1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107F1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10861462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10871462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10881462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10891462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108A1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108B1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108C1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108D1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108E1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10941462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10951462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10961462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10971462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10991462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_109A1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10A01462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10A11462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10A31462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10A41462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10A61462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10A71462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10AA1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10AC1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10AD1462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76411462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76671462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76701462&REV_06 ;MSI_CHANNEL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76721462&REV_06 ;MSI_CHANNEL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76731462&REV_06 ;MSI_CHANNEL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76761462&REV_06 ;MSI_CHANNEL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76781462&REV_06 ;MSI_CHANNEL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76801462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76811462&REV_06 ;MSI_CHANNEL
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76871462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76931462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_76981462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77131462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77151462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77161462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77181462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77201462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77301462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77311462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77321462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77351462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77411462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77451462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_77501462&REV_06 ;MSI
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89671033&REV_06 ;NEC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A0211BCF&REV_06 ;NEC
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_000313B8&REV_06 ;Nokia
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A2011B72&REV_06 ;OTS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A2021B72&REV_06 ;OTS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A2171B72&REV_06 ;OTS
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_833810F7&REV_06 ;Panasonic
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00031179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FC301179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FC661179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FC801179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FC821179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FD001179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FD301179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FD3C1179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FD691179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FD801179&REV_06 ;Toshiba
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004D14C0&REV_06 ;WB
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004E14C0&REV_06 ;WB
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_005014C0&REV_06 ;WB
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_005114C0&REV_06 ;WB
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_005214C0&REV_06 ;WB
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_005714C0&REV_06 ;WB
%RTL8168E.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_006114C0&REV_06 ;WB

; HP 8168E S5 WOL Default Disable
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA7103C ;HP_F01
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA8103C ;HP_ArnicaF02
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAB103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAC103C ;HP_Aronia
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAD103C ;HP_Anhui
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAE103C ;HP_Alberta
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AB5103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AB6103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABB103C ;HP_Inglewood
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABE103C ;HP_Hudson
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABF103C ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC2103C ;HP_Carmel
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC3103C ;HP_Lavaca
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC4103C ;HP_Angelino
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC5103C ;HP_Leon
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC8103C ;HP_Angelica
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACD103C ;HP_Hibiscus
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACE103C ;HP_Pittsburgh
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACF103C ;HP_Holly

; HP 8168E S5 WOL Hide and Default Enable
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1592103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1593103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1594103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1595103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1596103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1597103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1599103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_159A103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_159B103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1633103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1634103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1635103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164F103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1676103C&REV_06 ;HP_Metallica
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1677103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1678103C&REV_06 ;HP_Madonna
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167C103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167D103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167E103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167F103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1680103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168B103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168C103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168E103C&REV_06 ;HP
%RTL8168E.DeviceDesc%  = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168F103C&REV_06 ;HP

; 8168E EEE Default Enable
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15B110CF&REV_06 ;Fuji
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16AF10CF&REV_06 ;Fuji

; 8168E EEE Default Enable & S5 WOL Hide and Default Disable
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_907B104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_907E104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9083104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9084104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9085104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9086104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9087104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9088104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9089104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_908B104D&REV_06 ;SONY
%RTL8168E.DeviceDesc%  = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_908E104D&REV_06 ;SONY

; 8168ES
%RTL8168E.DeviceDesc%  = RTL8168ES.ndi, PCI\VEN_10EC&DEV_8168&REV_08
%RTL8168E.DeviceDesc%  = RTL8168ES.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_08


; 8104
%RTL8104.DeviceDesc%  = RTL8104.ndi, PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%  = RTL8104.ndi, PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03


; 8401
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_04
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_04
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_044A1028&REV_04 ;DELL
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_044B1028&REV_04 ;DELL
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_04 ;Toshiba
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_04 ;Toshiba
%RTL8401.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_07711558&REV_04 ;Clevo

; HP 8401 S5 WOL Hide and Default Enable
%RTL8401.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1404103C&REV_04 ;HP
%RTL8401.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1406103C&REV_04 ;HP
%RTL8401.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_140A103C&REV_04 ;HP
%RTL8401.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1415103C&REV_04 ;HP
%RTL8401.DeviceDesc%  = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_148A103C&REV_04 ;HP

; 8105E
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&REV_05
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_05
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_043D1025&REV_05 ;Acer
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_058F1025&REV_05 ;Acer
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05901025&REV_05 ;Acer
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_A2141B72&REV_05 ;AOC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_105C1043&REV_05 ;ASUS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_046B1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_046C1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_046D1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_046E1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04721028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_048B1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_048E1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04AF1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04B01028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04B11028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04B21028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04B31028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C11028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C21028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C31028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C41028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C51028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C61028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04C91028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04CA1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04CB1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04CC1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04CD1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D01028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D11028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D21028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D31028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D41028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D51028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D71028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D81028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04D91028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04DA1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04EF1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04F01028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04F11028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04F21028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04F31028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_04F41028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05021028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05031028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05041028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05051028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05061028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05071028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05081028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05131028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_051C1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_051D1028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_05261028&REV_05 ;DELL
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_22DA1019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_81051019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99821019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99CD1019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99D21019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99D41019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99D51019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99D81019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_99DB1019&REV_05 ;ECS
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50181509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50191509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50201509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50231509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50261509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50271509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50281509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50291509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50301509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50311509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50321509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50331509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50341509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50351509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50361509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50371509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50381509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50391509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_50401509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60501509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60511509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60521509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60531509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60541509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60551509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60561509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60571509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60581509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60591509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_60601509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_70041509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_70051509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_70061509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_70081509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_70091509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80241509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80251509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80261509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80271509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80281509&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_A214160B&REV_05 ;FIC
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D72105B&REV_05 ;FOXCONN_Clone
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0D78105B&REV_05 ;FOXCONN_Clone
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E28105B&REV_05 ;FOXCONN_Clone
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_0E39105B&REV_05 ;FOXCONN_Clone
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_020010CF&REV_05 ;Fuji
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_15B110CF&REV_05 ;Fuji
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_311510CF&REV_05 ;Fuji
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10E417C0&REV_05 ;Generic
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_165C103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_165D103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_165E103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_165F103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1660103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1661103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1662103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1663103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1664103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1665103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1666103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1667103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1668103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1669103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_166A103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_166B103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_166C103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_166D103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_166E103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_166F103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1670103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1671103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1672103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1693103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1694103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1695103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1696103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1697103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1698103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1699103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_169A103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_169B103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_169C103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1775103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1776103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3387103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_338A103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_338B103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_338C103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_338D103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3393103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3562103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3563103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3564103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3565103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3566103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3567103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3568103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3569103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3577103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3578103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3579103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_357A103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3594103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3672103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3673103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3674103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3675103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_3676103C ;HP
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_397517AA&REV_05 ;Lenovo
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10A11462&REV_05 ;MSI
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_10AD1462&REV_05 ;MSI
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_00041179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC301179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC661179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC671179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC761179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC771179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC801179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC821179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FC901179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD001179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD301179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD3C1179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD691179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD6A1179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD6B1179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD791179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD7A1179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD7B1179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FD801179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FDA01179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FDB01179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FDC01179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF1E1179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_05 ;Toshiba
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_005814C0&REV_05 ;WB
%RTL8105.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_006114C0&REV_05 ;WB

; HP 8105E S5 WOL Default Disable
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA7103C ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA8103C ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA9103C ;HP_Alpinia
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AAD103C ;HP_Anhui
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AAE103C ;HP_Alberta
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AAF103C ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB1103C ;HP_Alvorix
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB4103C ;HP_Inverness
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB7103C ;HP_Apricot
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABA103C ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABC103C ;HP_Arrowwood
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABD103C ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABF103C ;HP_Cupertino
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AC2103C ;HP_Carmel
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AC7103C ;HP_Armand
%RTL8105.DeviceDesc%  = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ACA103C ;HP

; HP 8105E S5 WOL Hide and Default Enable
%RTL8105.DeviceDesc%  = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1584103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1585103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1676103C&REV_05 ;HP
%RTL8105.DeviceDesc%  = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1678103C&REV_05 ;HP

; HP 8105E S5 WOL Hide and Default Disable
%RTL8105.DeviceDesc%  = RTL8105S5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1586103C&REV_05 ;HP

; 8105E EEE Default Enable
%RTL8105.DeviceDesc%  = RTL8105EEEEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_162A10CF&REV_05 ;Fuji


; 8168F
%RTL8168F.DeviceDesc%  = RTL8168F.ndi, PCI\VEN_10EC&DEV_8168&REV_07
%RTL8168F.DeviceDesc%  = RTL8168F.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_07


; Realtek
;
; Windows NT specific entry

[R8169C7k.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, JumboNolimit.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8169.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe4k.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136HP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = AutoCrossoverDet.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136HPS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5woldefaultdisable.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = AutoCrossoverDet.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168C.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthDisabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthDisabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CNotSpdDown.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolS5LinkSpeedNotSpdDown.reg, GreenEthDisabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CForceGigabit.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed1g.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolS5LinkSpeedForce1g.reg, GreenEthDisabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CForce100Full.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = SpeedForce100Full.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthDisabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dellsov1_8102.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102S5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dellsov1_8102.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102S5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dellsov1_8102.reg, dels5wol.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102ForceEnableClkReq.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dellsov1_8102.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, ForceEnableClkReq.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168D.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168DS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168DS5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168DP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168E.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168ES5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168ES5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168EEEEEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEEnable.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168EEEEEnS5WOLHideDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhidedisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEEnable.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168ES.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168F.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3 

[RTL8104.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = WolShutdownLinkSpeed.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105S5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105S5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105S5WOLHideDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhidedisable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105EEEEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEEnable.reg
AddReg          = about.reg
CopyFiles       = RTL8167.CopyFiles, RTLDLL.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3


[R8169C7k.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8169.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8136.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8136HP.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8136HPS5WOLDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168C.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168CS5WOLDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168CNotSpdDown.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168CForceGigabit.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168CForce100Full.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8102.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8102S5WOLDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8102S5WOLHideEnable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8102ForceEnableClkReq.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168D.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168DS5WOLDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168DS5WOLHideEnable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168DP.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168E.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168ES5WOLDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168ES5WOLHideEnable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168EEEEEnable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168ES.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8168F.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8104.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8105.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8105S5WOLDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8105S5WOLHideEnable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8105S5WOLHideDisable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles

[RTL8105EEEEnable.ndi.NT.CoInstallers]
AddReg          = RTNUninst.reg
CopyFiles       = RTNUninst.CopyFiles


[RTL8168.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8136.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8136HP.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8136HPS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168C.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168CS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168CNotSpdDown.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168CForceGigabit.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168CForce100Full.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8102.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8102S5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8102S5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8102ForceEnableClkReq.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168D.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168DS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168DS5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168DP.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168E.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168ES5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168ES5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168EEEEEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168ES.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8168F.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8104.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8105.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8105S5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8105S5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8105S5WOLHideDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg

[RTL8105EEEEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg


[RTL8168_8136.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[RTL8168D.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1


[R8169C7k.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8169.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8136.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8136HP.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8136HPS5WOLDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168C.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168CS5WOLDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168CNotSpdDown.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168CForceGigabit.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168CForce100Full.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8102.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8102S5WOLDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8102S5WOLHideEnable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8102ForceEnableClkReq.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168D.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168DS5WOLDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168DS5WOLHideEnable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168DP.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168E.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168ES5WOLDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168ES5WOLHideEnable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168EEEEEnable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168ES.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8168F.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8104.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8105.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8105S5WOLDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8105S5WOLHideEnable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8105S5WOLHideDisable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog

[RTL8105EEEEnable.ndi.NT.Services]
AddService = RTL8167, 2, rtl8167.Service, common.EventLog



;-----------------------------------------------------------------------------
; common base for 10/100/1000 Mb Adapters
;
[Common.reg]
HKR,,DeviceRemovable,0,"0" 

HKR,,HwParaMask,0x00010001,0 

HKR,,HwOptimize,0x00010001,0 

HKR,,HwOption,0x00010001,0 

HKR,,LogDisconnectEvent,0,"0" 

HKR,,EnableEDT,0,"1"

HKR,,RIACP,0,"0"

HKR,,S5NicKeepOverrideMacAddr,0,"0"

HKR,,PPSW,0,"1"

HKR,,S0MgcPkt,0,"0"

HKR,,HwFPSM,0x00010001,0

HKR,,SwIML,0x00010001,0

HKR,,ENPWMode,0,"0"

HKR,,Diskless,0,"0"

HKR,,TxOptimizeThreshold,0x00010001,0

HKR,,RxOptimizeThreshold,0x00010001,0

[Speed.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

HKR,Ndi\params\AutoDisableGigabit,       ParamDesc,  0, %AutoDisableGigabit%
HKR,Ndi\params\AutoDisableGigabit,       default,    0, "0"
HKR,Ndi\params\AutoDisableGigabit,       type,       0, "enum"
HKR,Ndi\params\AutoDisableGigabit\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoDisableGigabit\enum,  "1",        0, %BatteryRe-Link%
HKR,Ndi\params\AutoDisableGigabit\enum,  "2",        0, %AcBatteryRe-Link%
HKR,,AutoDisableGigabit,0,"0"

[Speed1g.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "6"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"6"

HKR,,ForceMode,0,"0"

[Speed10_100.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[SpeedForce100Full.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"4"

HKR,,ForceMode,0,"1"

[about.reg]
HKR,,EnumPropPages32,,"rtnicprop64.dll,RTNicPropPageProvider"

[RTNUninst.reg]
HKR,,CoInstallers32,0x00010000,"RTNUninst64.dll,RTNUninst"

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	   ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	   type,       0, "edit"
HKR,Ndi\params\NetworkAddress,	   default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,	   LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,	   UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,	   Optional,   0, "1"

[flowctrl.reg]
HKR,Ndi\params\*FlowControl,	   ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,	   default,    0, "1"
HKR,Ndi\params\*FlowControl,	   type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "1",        0, %Enabled%
HKR,,*FlowControl,0,"1"


[PriorityVlanTag.reg]
HKR,Ndi\params\*PriorityVLANTag,	ParamDesc,  0, %PriorityVLAN%
HKR,Ndi\params\*PriorityVLANTag,	default,    0, "0"
HKR,Ndi\params\*PriorityVLANTag,	type,       0, "enum"
HKR,Ndi\params\*PriorityVLANTag\enum,	"0",        0, %PriorityVLANDisabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"1",        0, %PriorityEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"2",        0, %VLANEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"3",        0, %PriorityVLANEnabled%
HKR,,*PriorityVLANTag,0,"3"

[InterruptModeration.reg]
HKR,Ndi\params\*InterruptModeration,	ParamDesc,  0, %InterruptModeration%
HKR,Ndi\params\*InterruptModeration,	default,    0, "1"
HKR,Ndi\params\*InterruptModeration,	type,       0, "enum"
HKR,Ndi\params\*InterruptModeration\enum,	"0",        0, %Disabled%
HKR,Ndi\params\*InterruptModeration\enum,	"1",        0, %Enabled%
HKR,,*InterruptModeration,0,"1"

[TxRxBuf.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[Jumboframe.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe4k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe9k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "8192",     0, %8KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "9216",     0, %9KBMTU%
HKR,,*JumboPacket,0,"1514"

[JumboNolimit.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"
HKR,,LimitCbJumboFrame,0,"0"

[Offload.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadChksum.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

[s5wol.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[s5woldefaultdisable.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "0"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"0"

[s5wolhideenable.reg]
HKR,,S5WakeOnLan,0,"1"

[s5wolhidedisable.reg]
HKR,,S5WakeOnLan,0,"0"

[OffloadIpv6Lsov2.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,	ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,	default,    0, "0"
HKR,Ndi\params\*LsoV2IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"0"

HKR,Ndi\params\*LsoV2IPv6,	ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

HKR,Ndi\params\*RSS,	ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,	default,    0, "1"
HKR,Ndi\params\*RSS,	type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"1"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",       0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",       0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadIpv6Lsov2_8102.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*RSS,	ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,	default,    0, "1"
HKR,Ndi\params\*RSS,	type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"1"

HKR,Ndi\params\*LsoV2IPv4,	ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"1"

HKR,Ndi\params\*LsoV2IPv6,	ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,	ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,	default,    0, "0"
HKR,Ndi\params\AutoCrossoverDet,	type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

[WolShutdownLinkSpeed.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	default,    0, "0"
HKR,Ndi\params\WolShutdownLinkSpeed,	type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"0"

[WolS5LinkSpeedNotSpdDown.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,	type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolS5LinkSpeedForce1g.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,	type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[wolptnmagic.reg]
HKR,Ndi\params\*WakeOnPattern,  ParamDesc,  0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,	default,    0, "1"
HKR,Ndi\params\*WakeOnPattern,	type,       0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,   "1",        0, %Enabled%
HKR,,*WakeOnPattern,0,"1"

HKR,Ndi\params\*WakeOnMagicPacket,	ParamDesc,  0, %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,	default,    0, "1"
HKR,Ndi\params\*WakeOnMagicPacket,	type,       0, "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*WakeOnMagicPacket,0,"1"

[GreenEthEnabled.reg]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "1"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"1"

[GreenEthDisabled.reg]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "0"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"0"

[ArpNsProtOffload.reg]
HKR,Ndi\params\*PMARPOffload,       ParamDesc,  0, %ArpOffload%
HKR,Ndi\params\*PMARPOffload,	    default,    0, "1"
HKR,Ndi\params\*PMARPOffload,	    type,       0, "enum"
HKR,Ndi\params\*PMARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*PMARPOffload\enum,  "1",        0, %Enabled%
HKR,,*PMARPOffload,0,"1"

HKR,Ndi\params\*PMNSOffload,	    ParamDesc,  0, %NsOffload%
HKR,Ndi\params\*PMNSOffload,	    default,    0, "1"
HKR,Ndi\params\*PMNSOffload,	    type,       0, "enum"
HKR,Ndi\params\*PMNSOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*PMNSOffload\enum,   "1",        0, %Enabled%
HKR,,*PMNSOffload,0,"1"

[EEE.reg]
HKR, Ndi\params\EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\EEE,        type,       0, "enum"
HKR, Ndi\params\EEE,        default,    0, "1"
HKR, Ndi\params\EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EEE\enum,   "1",        0, %Enabled%
HKR,,EEE,0,"1"

[EEEEnable.reg]
HKR, Ndi\params\EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\EEE,        type,       0, "enum"
HKR, Ndi\params\EEE,        default,    0, "1"
HKR, Ndi\params\EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EEE\enum,   "1",        0, %Enabled%
HKR,,EEE,0,"1"

[HDSplit.reg]
HKR,Ndi\params\*HeaderDataSplit,	ParamDesc,  0, %HDSplit%
HKR,Ndi\params\*HeaderDataSplit,	default,    0, "1"
HKR,Ndi\params\*HeaderDataSplit,	type,       0, "enum"
HKR,Ndi\params\*HeaderDataSplit\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*HeaderDataSplit\enum,   "1",        0, %Enabled%
HKR,,*HeaderDataSplit,0,"1"

;HKR,,PnPCapabilities,0x10001,0x0000

[PDPllDisabled.reg]
HKR,,PowerDownPll,0,"0"

[PDPllEnabled.reg]
HKR,,PowerDownPll,0,"1"

[DisablePBA.reg]
HKR,,DisablePBA,0,"1"

[EnablePBA.reg]
HKR,,DisablePBA,0,"0"

[ForceEnableClkReq.reg]
HKR,,ForceEnableClkReq,0,"1"


[del.reg]
HKR,Ndi\params\JumboFrame
HKR,,JumboFrame

HKR,Ndi\params\S3S4WolPowerSaving
HKR,,S3S4WolPowerSaving

HKR,,PowerDownPll

[dellsov1_8102.reg]
HKR,Ndi\params\*LsoV1IPv4
HKR,,*LsoV1IPv4

[dels5wol.reg]
HKR,Ndi\params\S5WakeOnLan
HKR,,S5WakeOnLan


;-----------------------------------------------------------------------------
; rtk NT specific
;

[rtk.reg]
HKR, Ndi,                       Service,    0, "RTL8167"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"


[rtl8167.Service]
DisplayName     = %rtl8167.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rt64win7.sys
LoadOrderGroup  = NDIS


[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\Rt64win7.sys"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; DestinationDirs
;
[RTL8167.CopyFiles]
Rt64win7.sys,,,2

[RTLDLL.CopyFiles]
RtNicProp64.dll,,,0x00006000 ; COPYFLG_NOPRUNE | COPYFLG_IN_USE_RENAME

[RTNUninst.CopyFiles]
RTNUninst64.dll,,,0x00006000 ; COPYFLG_NOPRUNE | COPYFLG_IN_USE_RENAME

[SourceDisksNames]
1 = %DiskDescription%


[SourceDisksFiles]
Rt64win7.sys = 1,, ; on distribution disk 1
RtNicProp64.dll = 1,, ; on distribution disk 1
RTNUninst64.dll = 1,, ; on distribution disk 1


[DestinationDirs]
RTL8167.CopyFiles  = 12
DefaultDestDir     = 11

[Strings]
Realtek                  = "Realtek"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
NetworkAddress		 = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
AutoDisableGigabit       = "Auto Disable Gigabit"
AutoLinkDownPhyOff       = "Auto Disable PHY"
BatteryRe-Link           = "Re-Link, Battery"
AcBatteryRe-Link         = "Re-Link, Battery or AC"
Battery                  = "Enabled, Battery"
AcBattery                = "Enabled, Battery or AC"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Auto Disable PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Auto Crossover Detection"
PriorityEnabled          = "Priority Enabled"
VLANEnabled              = "VLAN Enabled"
10MbFirst                = "10 Mbps First"
100MbFirst               = "100 Mbps First"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Arabic_UAX
[Strings.3801]
Realtek                  = "Realtek"

AutoDetect               = "التفاوض التلقائي"
SpeedDuplex              = "السرعة والازدواج"
10Mb-Half-Duplex         = "نصف المزدوج 10 ميجا بايت في الثانية"
10Mb-Full-Duplex         = "كامل الازدواج 10 ميجا بايت في الثانية"
100Mb-Half-Duplex        = "كامل الازدواج 100 ميجا بايت في الثانية"
100Mb-Full-Duplex        = "كامل الازدواج 100 ميجا بايت في الثانية" 
1000Mb-Full-Duplex       = "كامل الازدواج 1000 ميجا بايت في الثانية"
NetworkAddress		 = "عنوان الشبكة"
IPChksumOffv4            = "تحميل المجموع الاختباري IPv4"
TCPChksumOffv4           = "تحميل المجموع الاختباري IPv4) TCP)"
UDPChksumOffv4           = "تحميل المجموع الاختباري IPv4) UDP)"
TCPChksumOffv6           = "تحميل المجموع الاختباري IPv6) TCP)"
UDPChksumOffv6           = "تحميل المجموع الاختباري IPv6) UDP)"
Enabled                  = "قيد التمكين"
Disabled                 = "قيد التعطيل"
TxEnabled                = "Tx قيد التمكين"
RxEnabled                = "Rx قيد التمكين"
RxTxEnabled              = "Rx & Tx قيد التمكين"
LSOv4                    = "تحميل الإرسال الكبير (IPv4)"
LSOv2v4                  = "تحميل الإرسال الكبير IPv4) v2)"
LSOv2v6                  = "تحميل الإرسال الكبير IPv6) v2)"
FlowControl              = "التحكم بالانسياب"
PriorityVLAN             = "الأولوية وVLAN"
PriorityVLANDisabled     = "الأولوية وVLAN قيد التعطيل"
PriorityVLANEnabled      = "الأولوية وVLAN قيد التمكين"
InterruptModeration      = "قطع التوسط"
ReceiveBuffers           = "استقبال المخزنات المؤقتة"
TransmitBuffers          = "نقل المخزنات المؤقتة"
AutoDisableGigabit       = "تعطيل تلقائي جيجا بت (PowerSaving)"
AutoLinkDownPhyOff       = "تعطيل تلقائي PowerSaving) PHY)"
BatteryRe-Link           = "إعادة الربط، البطارية"
AcBatteryRe-Link         = "إعادة الربط، البطارية أو التيار المتردد"
Battery                  = "قيد التمكين، البطارية"
AcBattery                = "قيد التمكين، البطارية أو التيار المتردد"
JumboFrame               = "الإطار الضخم"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "إغلاق معيار Wake-On-Lan"
AutoLinkDownPcieMacOff   = "تعطيل تلقائي PowerSaving) PCIe)"
RSS                      = "استلام تحديد مقياس الجانب"
AutoCrossoverDet         = "رصد التحويل التلقائي"
PriorityEnabled          = "الأولوية قيد التمكين"
VLANEnabled              = "VLAN قيد التمكين"
10MbFirst                = "10 ميجا بايت في الثانية أولا"
100MbFirst               = "100 ميجا بايت في الثانية أولا"
WolShutdownLinkSpeed     = "رابط السرعة للإغلاق وWOL"
NotSpeedDown             = "عدم تخفيض السرعة"
WolCap                   = "قدرات تنشيط Lan"
None                     = "لا شيء"
PatternMatch             = "مطابقة عامل البحث"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "مطابقة عامل البحث وMagic Packet"
GreenEthernet            = "إيثرنت أخضر"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Chinese_Taiwan
[Strings.0404]
Realtek                  = "Realtek"

AutoDetect               = "自動偵測"
SpeedDuplex              = "連線速度與雙工模式"
10Mb-Half-Duplex         = "10 Mbps 半雙工"
10Mb-Full-Duplex         = "10 Mbps 全雙工"
100Mb-Half-Duplex        = "100 Mbps 半雙工"
100Mb-Full-Duplex        = "100 Mbps 全雙工"
1000Mb-Full-Duplex       = "1.0 Gbps 全雙工"
NetworkAddress		 = "網路卡位址"
IPChksumOffv4            = "IPv4 檢查總和值卸載"
TCPChksumOffv4           = "TCP 檢查總和卸載 (IPv4)"
UDPChksumOffv4           = "UDP 檢查總和卸載 (IPv4)"
TCPChksumOffv6           = "TCP 檢查總和卸載 (IPv6)"
UDPChksumOffv6           = "UDP 檢查總和卸載 (IPv6)"
Enabled                  = "開啟"
Disabled                 = "關閉"
TxEnabled                = "Tx 開啟"
RxEnabled                = "Rx 開啟"
RxTxEnabled              = "Rx & Tx 開啟"
LSOv4                    = "大量傳送卸載 (IPv4)"
LSOv2v4                  = "大量傳送卸載 v2 (IPv4)"
LSOv2v6                  = "大量傳送卸載 v2 (IPv6)"
FlowControl              = "流量控制"
PriorityVLAN             = "優先權 & VLAN"
PriorityVLANDisabled     = "優先權 & VLAN 關閉"
PriorityVLANEnabled      = "優先權 & VLAN 開啟"
InterruptModeration      = "中斷調整合適化"
ReceiveBuffers           = "接收緩衝區"
TransmitBuffers          = "傳送緩衝區"
AutoDisableGigabit       = "自動關閉 Gigabit"
AutoLinkDownPhyOff       = "自動關閉 PHY"
BatteryRe-Link           = "重新連線, 電池"
AcBatteryRe-Link         = "重新連線, 電池或 AC"
Battery                  = "開啟, 電池"
AcBattery                = "開啟, 電池或 AC"
JumboFrame               = "巨大訊框"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "關機網路喚醒"
AutoLinkDownPcieMacOff   = "自動關閉 PCIe"
RSS                      = "接收端調整"
AutoCrossoverDet         = "自動跳線偵測"
PriorityEnabled          = "優先權開啟"
VLANEnabled              = "VLAN 開啟"
10MbFirst                = "10 Mbps 優先"
100MbFirst               = "100 Mbps 優先"
WolShutdownLinkSpeed     = "WOL & 關機連線速度"
NotSpeedDown             = "不降速"
WolCap                   = "網路喚醒能力"
None                     = "無"
PatternMatch             = "樣式比對"
MagicPacket              = "魔術封包"
PatternAndMagic          = "樣式比對及魔術封包"
GreenEthernet            = "環保節能"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Chinese (PRC)
[Strings.0804]
Realtek                  = "Realtek"

AutoDetect               = "自动侦测"
SpeedDuplex              = "连接速度和双工模式"
 
10Mb-Half-Duplex         = "10 Mbps 半双工"
10Mb-Full-Duplex         = "10 Mbps 全双工"
100Mb-Half-Duplex        = "100 Mbps 半双工"
100Mb-Full-Duplex        = "100 Mbps 全双工"
1000Mb-Full-Duplex       = "1.0 Gbps 全双工"
NetworkAddress		 = "网络地址"
IPChksumOffv4            = "IPv4 硬件校验和"
TCPChksumOffv4           = "TCP 硬件校验和 (IPv4)"
UDPChksumOffv4           = "UDP 硬件校验和 (IPv4)"
TCPChksumOffv6           = "TCP 硬件校验和 (IPv6)"
UDPChksumOffv6           = "UDP 硬件校验和 (IPv6)"
Enabled                  = "开启"
Disabled                 = "关闭"
TxEnabled                = "Tx 开启"
RxEnabled                = "Rx 开启"
RxTxEnabled              = "Rx & Tx 开启"
LSOv4                    = "大量传送减负 (IPv4)"
LSOv2v4                  = "大量传送减负 v2 (IPv4)"
LSOv2v6                  = "大量传送减负 v2 (IPv6)"
FlowControl              = "流控制"
PriorityVLAN             = "优先级和VLAN"
PriorityVLANDisabled     = "优先级和VLAN 关闭"
PriorityVLANEnabled      = "优先级和VLAN 开启"
InterruptModeration      = "中断调整"
ReceiveBuffers           = "接收缓冲区"
TransmitBuffers          = "传送缓冲区"
AutoDisableGigabit       = "自动关闭 Gigabit"
AutoLinkDownPhyOff       = "自动关闭 PHY"
BatteryRe-Link           = "重新联接, 电池"
AcBatteryRe-Link         = "重新联接, 电池或者交流电源"
Battery                  = "开启, 电池"
AcBattery                = "开启, 电池或者交流电源"
JumboFrame               = "巨型帧"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "关机 网络唤醒"
AutoLinkDownPcieMacOff   = "自动关闭 PCIe"
RSS                      = "接收端调整"
AutoCrossoverDet         = "自动跳线侦测"
PriorityEnabled          = "优先级开启"
VLANEnabled              = "VLAN 开启"
10MbFirst                = "10 Mbps 优先"
100MbFirst               = "100 Mbps 优先"
WolShutdownLinkSpeed     = "网络唤醒和关机连接速度"
NotSpeedDown             = "不降速"
WolCap                   = "网络唤醒能力"
None                     = "无"
PatternMatch             = "样式比对"
MagicPacket              = "魔术封包"
PatternAndMagic          = "样式比对及魔术封包"
GreenEthernet            = "环保节能"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Croatian
[Strings.041a]
Realtek                  = "Realtek"
AutoDetect               = "Automatsko prilagođivanje"
SpeedDuplex              = "Brzina i dupleks"
10Mb-Half-Duplex         = "10 Mb/s poludupleks"
10Mb-Full-Duplex         = "10 Mb/s puni dupleks"
100Mb-Half-Duplex        = "100 Mb/s poludupleks"
100Mb-Full-Duplex        = "100 Mb/s puni dupleks"
1000Mb-Full-Duplex       = "1.0 Gb/s puni dupleks"
NetworkAddress		 = "Mrežna adresa"
IPChksumOffv4            = "IPv4 kontrolni zbroj bez opterećenja"
TCPChksumOffv4           = "TCP kontrolni zbroj na periferiju (IPv4)"
UDPChksumOffv4           = "UDP kontrolni zbroj na periferiju (IPv4)"
TCPChksumOffv6           = "TCP kontrolni zbroj na periferiju (IPv6)"
UDPChksumOffv6           = "UDP kontrolni zbroj na periferiju (IPv6)"
Enabled                  = "Omogućeno"
Disabled                 = "Onemogućeno"
TxEnabled                = "Tx omogućeno"
RxEnabled                = "Rx omogućeno"
RxTxEnabled              = "Rx & Tx omogućeno"
LSOv4                    = "Slanje velikog na periferiju (IPv4)"
LSOv2v4                  = "Slanje velikog na periferiju v2 (IPv4)"
LSOv2v6                  = "Slanje velikog na periferiju v2 (IPv6)"
FlowControl              = "Kontrola protoka"
PriorityVLAN             = "Prioritet i VLAN"
PriorityVLANDisabled     = "Prioritet i VLAN onemogućen"
PriorityVLANEnabled      = "Prioritet i VLAN omogućeni"
InterruptModeration      = "Moderacija prekida"
ReceiveBuffers           = "Spremnici prijema"
TransmitBuffers          = "Spremnici prijenosa"
AutoDisableGigabit       = "Automatsko isključivanje Gigabita"
AutoLinkDownPhyOff       = "Automatsko isključivanje PHY"
BatteryRe-Link           = "Re-Link, baterija"
AcBatteryRe-Link         = "Re-Link, baterija ili AC napajanje"
Battery                  = "Omogućeno, baterija"
AcBattery                = "Omogućeno, baterije ili AC"
JumboFrame               = "Jumbo okvir"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Isključivanje funkcije Probudi se na mreži nakon isključivanja"
AutoLinkDownPcieMacOff   = "Automatsko isključivanje PCIe"
RSS                      = "Smanjivanje na strani prijema"
AutoCrossoverDet         = "Automatska detekcija preslušavanja"
PriorityEnabled          = "Prioritet omogućen"
VLANEnabled              = "VLAN omogućen"
10MbFirst                = "Prvo 10 Mb/s"
100MbFirst               = "Prvo 100 Mb/s"
WolShutdownLinkSpeed     = "Brzina veze za WOL i isključivanje"
NotSpeedDown             = "Nema smanjivanja brzine"
WolCap                   = "Mogućnosti Probudi se na mreži"
None                     = "Nema"
PatternMatch             = "Podudarnost obrasca"
MagicPacket              = "Magični paket"
PatternAndMagic          = "Podudarnost obrasca i magični paket"
GreenEthernet            = "Zeleni Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; CZ
[Strings.0405]
Realtek                  = "Realtek"

AutoDetect               = "Automatické nastavení režimu provozu"
SpeedDuplex              = "Rychlost a přenosový režim"
10Mb-Half-Duplex         = "Poloduplexní 10 Mbps"
10Mb-Full-Duplex         = "Plně duplexní 10 Mbps"
100Mb-Half-Duplex        = "Poloduplexní 100 Mbps"
100Mb-Full-Duplex        = "Plně duplexní 100 Mbps"
1000Mb-Full-Duplex       = "Plně duplexní 1,0 Gbps"
NetworkAddress		 = "Síťová adresa"
IPChksumOffv4            = "Výpočet kontrolních součtů protokolu IPv4"
TCPChksumOffv4           = "Výpočet kontrolních součtů protokolu TCP (IPv4)"
UDPChksumOffv4           = "Výpočet kontrolních součtů protokolu UDP (IPv4)"
TCPChksumOffv6           = "Výpočet kontrolních součtů protokolu TCP (IPv6)"
UDPChksumOffv6           = "Výpočet kontrolních součtů protokolu UDP (IPv6)"
Enabled                  = "Povoleno"
Disabled                 = "Zakázáno"
TxEnabled                = "Odesílání povoleno"
RxEnabled                = "Příjem povolen"
RxTxEnabled              = "Příjem a odesílání povoleno"
LSOv4                    = "Zpracování velkých segmentů LSO (IPv4)"
LSOv2v4                  = "Zpracování velkých segmentů LSO v2 (IPv4)"
LSOv2v6                  = "Zpracování velkých segmentů LSO v2 (IPv6)"
FlowControl              = "Řízení toku"
PriorityVLAN             = "Priorita a VLAN"
PriorityVLANDisabled     = "Priorita a VLAN zakázána"
PriorityVLANEnabled      = "Priorita a VLAN povolena"
InterruptModeration      = "Tlumení přerušení"
ReceiveBuffers           = "Zásobníky příjmu"
TransmitBuffers          = "Zásobníky odesílání"
AutoDisableGigabit       = "Automatická deaktivace gigabitové sítě"
AutoLinkDownPhyOff       = "Automatická deaktivace PHY"
BatteryRe-Link           = "Re-link, baterie"
AcBatteryRe-Link         = "Re-link, baterie nebo AC"
Battery                  = "Povoleno, baterie"
AcBattery                = "Povoleno, baterie nebo AC"
JumboFrame               = "Jumbo rámec"
2KBMTU                   = "2 KB MTU"
3KBMTU                   = "3 KB MTU"
4KBMTU                   = "4 KB MTU"
5KBMTU                   = "5 KB MTU"
6KBMTU                   = "6 KB MTU"
7KBMTU                   = "7 KB MTU"
8KBMTU                   = "8 KB MTU"
9KBMTU                   = "9 KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Automatická deaktivace PCIe"
RSS                      = "Škálování na straně příjmu"
AutoCrossoverDet         = "Automatická detekce křížených kabelů"
PriorityEnabled          = "Priorita povolena"
VLANEnabled              = "VLAN povolena"
10MbFirst                = "Nejdříve 10 Mbps"
100MbFirst               = "Nejdříve 100 Mbps"
WolShutdownLinkSpeed     = "Rychlost linky pro WOL a vypnutí"
NotSpeedDown             = "Bez zpomalení"
WolCap                   = "Možnosti zapnutí počítače přes síť"
None                     = "Žádný"
PatternMatch	         = "Shoda řetězce"
MagicPacket	             = "Magic Packet"
PatternAndMagic          = "Shoda řetězce a Magic Packet"
GreenEthernet            = "Zelený Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Danish
[Strings.0406]
Realtek                  = "Realtek"

AutoDetect               = "Automatisk forhandling"
SpeedDuplex              = "Hastighed og duplex"
10Mb-Half-Duplex         = "10 Mbps halv duplex"
10Mb-Full-Duplex         = "10 Mbps fuld duplex"
100Mb-Half-Duplex        = "100 Mbps halv duplex"
100Mb-Full-Duplex        = "100 Mbps fuld duplex"
1000Mb-Full-Duplex       = "1.0 Gbps fuld duplex"
NetworkAddress           = "Netværksadresse"
IPChksumOffv4            = "Aflastning af IPv4 kontrolsum"
TCPChksumOffv4           = "Aflastning af TCP kontrolsum (IPv4)"
UDPChksumOffv4           = "Aflastning af UDP kontrolsum (IPv4)"
TCPChksumOffv6           = "Aflastning af TCP kontrolsum (IPv6)"
UDPChksumOffv6           = "Aflastning af UDP kontrolsum (IPv6)"
Enabled                  = "Aktiveret"
Disabled                 = "Deaktiveret"
TxEnabled                = "Tx aktiveret"
RxEnabled                = "Rx aktiveret"
RxTxEnabled              = "Rx og Tx aktiveret"
LSOv4                    = "Aflastning af stor forsendelse (IPv4)"
LSOv2v4                  = "Aflastning af stor forsendelse v2 (IPv4)"
LSOv2v6                  = "Aflastning af stor forsendelse v2 (IPv6)"
FlowControl              = "Flow-kontrol"
PriorityVLAN             = "Prioritet og VLAN"
PriorityVLANDisabled     = "Prioritet og VLAN deaktiveret"
PriorityVLANEnabled      = "Prioritet og VLAN aktiveret"
InterruptModeration      = "Interruptindstilling"
ReceiveBuffers           = "Modtagelsesbuffer"
TransmitBuffers          = "Afsendelsesbuffere"
AutoDisableGigabit       = "Automatisk deaktivering af gigabit"
AutoLinkDownPhyOff       = "Automatisk deaktivering af PHY"
BatteryRe-Link           = "Genetabler forbindelse, batteri"
AcBatteryRe-Link         = "Genetabler forbindelse, batteri eller AC"
Battery                  = "Aktiveret, batteri"
AcBattery                = "Aktiveret, batteri eller AC"
JumboFrame               = "Jumboramme"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Nedluk Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Automatisk deaktivering af PCIe"
RSS                      = "Skalering, modtagelsesside"
AutoCrossoverDet         = "Detektering af automatisk crossover"
PriorityEnabled          = "Prioritet aktiveret"
VLANEnabled              = "VLAN aktiveret"
10MbFirst                = "10 Mbps først"
100MbFirst               = "100 Mbps først"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Grøn Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Dutch
[Strings.0413]
Realtek                  = "Realtek"

AutoDetect               = "Automatisch onderhandelen"
SpeedDuplex              = "Snelheid & duplex"
10Mb-Half-Duplex         = "10 Mbps Half duplex"
10Mb-Full-Duplex         = "10 Mbps Full duplex"
100Mb-Half-Duplex        = "100 Mbps Half duplex"
100Mb-Full-Duplex        = "100 Mbps Full duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full duplex"
NetworkAddress           = "Netwerkadres"
IPChksumOffv4            = "IPv4-checksum-offload"
TCPChksumOffv4           = "TCP-checksum-offload (IPv4)"
UDPChksumOffv4           = "UDP-checksum-offload (IPv4)"
TCPChksumOffv6           = "TCP-checksum-offload (IPv6)"
UDPChksumOffv6           = "UDP-checksum-offload (IPv6)"
Enabled                  = "Ingeschakeld"
Disabled                 = "Uitgeschakeld"
TxEnabled                = "Tx ingeschakeld"
RxEnabled                = "Rx ingeschakeld"
RxTxEnabled              = "Rx & Tx ingeschakeld"
LSOv4                    = "Grote verzendings-offload (IPv4)"
LSOv2v4                  = "Grote verzendings-Offload v2 (IPv4)"
LSOv2v6                  = "Grote verzendings-Offload v2 (IPv6)"
FlowControl              = "Datatransportbesturing"
PriorityVLAN             = "Prioriteit & VLAN"
PriorityVLANDisabled     = "Prioriteit & VLAN uitgeschakeld"
PriorityVLANEnabled      = "Prioriteit & VLAN ingeschakeld"
InterruptModeration      = "Interrupt-controle"
ReceiveBuffers           = "Buffers ontvangst"
TransmitBuffers          = "Buffers verzending"
AutoDisableGigabit       = "Gigabit automatisch uitschakelen"
AutoLinkDownPhyOff       = "PHY automatisch uitschakelen"
BatteryRe-Link           = "Opnieuw verbinden, batterij"
AcBatteryRe-Link         = "Opnieuw verbinden, batterij of AC"
Battery                  = "Ingeschakeld, batterij"
AcBattery                = "Ingeschakeld, batterij of AC"
JumboFrame               = "Jumbo frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Wake-On-LAN uitschakelen"
AutoLinkDownPcieMacOff   = "PCIe automatisch uitschakelen"
RSS                      = "Schaling ontvangstzijde"
AutoCrossoverDet         = "Automatische kruislingse detectie"
PriorityEnabled          = "Prioriteit ingeschakeld"
VLANEnabled              = "VLAN ingeschakeld"
10MbFirst                = "10 Mbps eerst"
100MbFirst               = "100 Mbps eerst"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Patroonovereenkomst"
MagicPacket              = "Magisch pakket"
PatternAndMagic          = "Patroonovereenkomst & Magisch pakket"
GreenEthernet            = "Groen Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Finnish
[Strings.040B]
Realtek                  = "Realtek"

AutoDetect               = "Automaattinen neuvottelu"
SpeedDuplex              = "Nopeus & Duplex"
10Mb-Half-Duplex         = "10 Mbps puolikas Duplex"
10Mb-Full-Duplex         = "10 Mbps täysi Duplex"
100Mb-Half-Duplex        = "100 Mbps puolikas Duplex"
100Mb-Full-Duplex        = "100 Mbps täysi Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps täysi Duplex"
NetworkAddress           = "Verkon osoite"
IPChksumOffv4            = "IPv4 Pura tarkistussumma"
TCPChksumOffv4           = "TCP Pura tarkistussumma (IPv4)"
UDPChksumOffv4           = "UDP Pura tarkistussumma (IPv4)"
TCPChksumOffv6           = "TCP Pura tarkistussumma (IPv6)"
UDPChksumOffv6           = "UDP Pura tarkistussumma (IPv6)"
Enabled                  = "Käytössä"
Disabled                 = "Poistettu käytöstä"
TxEnabled                = "Tx Käytössä"
RxEnabled                = "Rx Käytössä"
RxTxEnabled              = "Rx & Tx Käytössä"
LSOv4                    = "Pura isot lähetykset (IPv4)"
LSOv2v4                  = "Pura isot lähetykset v2 (IPv4)"
LSOv2v6                  = "Pura isot lähetykset v2 (IPv6)"
FlowControl              = "Datavuon ohjaus"
PriorityVLAN             = "Etusija & VLAN"
PriorityVLANDisabled     = "Etusija & VLAN poistettu käytöstä"
PriorityVLANEnabled      = "Etusija & VLAN käytössä"
InterruptModeration      = "Keskeytyksen hidastaminen"
ReceiveBuffers           = "Vastaanota puskureita"
TransmitBuffers          = "Siirrä puskureita"
AutoDisableGigabit       = "Ota Gigabit automaattisesti pois päältä"
AutoLinkDownPhyOff       = "Ota PHY automaattisesti pois päältä"
BatteryRe-Link           = "Linkitä uudelleen, akku"
AcBatteryRe-Link         = "Linkitä uudelleen, akku tai verkkovirta"
Battery                  = "Käytössä, akku"
AcBattery                = "Käytössä, akku tai verkkovirta"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Sammuta herätystoiminto Lanin kautta"
AutoLinkDownPcieMacOff   = "Ota PCIe automaattisesti pois päältä"
RSS                      = "RSS-verkkosyötemuodot"
AutoCrossoverDet         = "Automaattinen ohitustunnistin"
PriorityEnabled          = "Etusija käytössä"
VLANEnabled              = "VLAN käytössä"
10MbFirst                = "10 Mbps ensin"
100MbFirst               = "100 Mbps ensin"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Vihreä Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; French
[Strings.040c]
Realtek                  = "Realtek"

AutoDetect               = "Négociation auto"
SpeedDuplex              = "Vitesse & Duplex"
10Mb-Half-Duplex         = "10 Mbps Semi-duplex"
10Mb-Full-Duplex         = "10 Mbps Duplex intégral"
100Mb-Half-Duplex        = "100 Mbps Semi-duplex"
100Mb-Full-Duplex        = "100 Mbps Duplex intégral"
1000Mb-Full-Duplex       = "1.0 Gbps Duplex intégral"
NetworkAddress           = "Adresse de réseau"
IPChksumOffv4            = "IPv4 Somme de contrôle hors charge"
TCPChksumOffv4           = "TCP Somme de contrôle hors charge (IPv4)"
UDPChksumOffv4           = "UDP Somme de contrôle hors charge (IPv4)"
TCPChksumOffv6           = "TCP Somme de contrôle hors charge (IPv6)"
UDPChksumOffv6           = "UDP Somme de contrôle hors charge (IPv6)"
Enabled                  = "Activé"
Disabled                 = "Désactivé"
TxEnabled                = "Tx activé"
RxEnabled                = "Rx activé"
RxTxEnabled              = "Rx & Tx activé"
LSOv4                    = "Grand envoi hors charge (IPv4)"
LSOv2v4                  = "Grand envoi hors charge v2 (IPv4)"
LSOv2v6                  = "Grand envoi hors charge v2 (IPv6)"
FlowControl              = "Contrôle de flux"
PriorityVLAN             = "Priorité & VLAN"
PriorityVLANDisabled     = "Priorité & VLAN désactivé"
PriorityVLANEnabled      = "Priorité & VLAN activé"
InterruptModeration      = "Modération interruption"
ReceiveBuffers           = "Mémoires tampon de réception"
TransmitBuffers          = "Mémoires tampon de transmission"
AutoDisableGigabit       = "Désactiver auto gigaoctet"
AutoLinkDownPhyOff       = "Désactiver auto PHY"
BatteryRe-Link           = "Re-lier, Batterie"
AcBatteryRe-Link         = "Re-lier, Batterie ou AC"
Battery                  = "Activé, Batterie"
AcBattery                = "Activé, Batterie ou AC"
JumboFrame               = "Cadre jumbo"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Arrêter Réveil par réseau"
AutoLinkDownPcieMacOff   = "Désactiver auto PCIe"
RSS                      = "Echelle coté réception"
AutoCrossoverDet         = "Détection auto inversion"
PriorityEnabled          = "Priorité activé"
VLANEnabled              = "VLAN activé"
10MbFirst                = "10 Mbps en premier"
100MbFirst               = "100 Mbps en premier"
WolShutdownLinkSpeed     = "WoL / Arrêt vitesse réseau"
NotSpeedDown             = "Pas vitesse ralentie"
WolCap                   = "Fonctions Réveil par le réseau"
None                     = "Aucun"
PatternMatch             = "Correspondance au modèle"
MagicPacket              = "Paquet Magic"
PatternAndMagic          = "Correspondance au modèle et Paquet Magic"
GreenEthernet            = "Ethernet vert"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; German
[Strings.0407]
Realtek                  = "Realtek"

AutoDetect               = "Autom. Aushandlung"
SpeedDuplex              = "Geschwindigkeit & Duplex"
10Mb-Half-Duplex         = "10 Mbit/s Halbduplex"
10Mb-Full-Duplex         = "10 Mbit/s Vollduplex"
100Mb-Half-Duplex        = "100 Mbit/s Halbduplex"
100Mb-Full-Duplex        = "100 Mbit/s Vollduplex"
1000Mb-Full-Duplex       = "1.0 Gbit/s Vollduplex"
NetworkAddress           = "Netzwerkadresse"
IPChksumOffv4            = "IPv4 Prüfsummenabladung"
TCPChksumOffv4           = "TCP Prüfsummenabladung (IPv4)"
UDPChksumOffv4           = "UDP Prüfsummenabladung (IPv4)"
TCPChksumOffv6           = "TCP Prüfsummenabladung (IPv6)"
UDPChksumOffv6           = "UDP-Prüfsummenabladung (IPv6)"
Enabled                  = "Aktiviert"
Disabled                 = "Deaktiviert"
TxEnabled                = "Tx aktiviert"
RxEnabled                = "Rx deaktiviert"
RxTxEnabled              = "Rx & Tx aktiviert"
LSOv4                    = "Abladung großer Übertragung (IPv4)"
LSOv2v4                  = "Abladung großer Übertragung V2 (IPv4)"
LSOv2v6                  = "Abladung großer Übertragung V2 (IPv6)"
FlowControl              = "Fließkontrolle"
PriorityVLAN             = "Priorität & VLAN"
PriorityVLANDisabled     = "Priorität & VLAN deaktiviert"
PriorityVLANEnabled      = "Priorität & VLAN aktiviert"
InterruptModeration      = "Interrupt-Moderation"
ReceiveBuffers           = "Puffer empfangen"
TransmitBuffers          = "Puffer übertragen"
AutoDisableGigabit       = "Gigabit autom. deaktivieren"
AutoLinkDownPhyOff       = "PHY autom. deaktivieren"
BatteryRe-Link           = "Wiederverbindung, Batterie"
AcBatteryRe-Link         = "Wiederverbindung, Batterie oder Netz"
Battery                  = "Aktiviert, Batterie"
AcBattery                = "Aktiviert, Batterie oder Netz"
JumboFrame               = "Jumbo-Rahmen"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Wake-On-Lan herunterfahren"
AutoLinkDownPcieMacOff   = "PCIe autom. deaktivieren"
RSS                      = "Seitenskalierung empfangen"
AutoCrossoverDet         = "Autom. Crossover-Erkennung"
PriorityEnabled          = "Priorität aktiviert"
VLANEnabled              = "VLAN aktiviert"
10MbFirst                = "10 Mbit/s zuerst"
100MbFirst               = "100 Mbit/s zuerst"
WolShutdownLinkSpeed     = "WoL / Link-Geschwindigkeit reduzieren"
NotSpeedDown             = "Nicht verlangsamen"
WolCap                   = "Wake-On-LAN-Funktionen"
None                     = "Kein"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green-Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Greek
[Strings.0408]
Realtek                  = "Realtek"

AutoDetect               = "Αυτόματη διαπραγμάτευση"
SpeedDuplex              = "Ταχύτητα & Αμφίδρομη"
10Mb-Half-Duplex         = "10Mbps/Ημι-αμφίδρομη"
10Mb-Full-Duplex         = "10Mbps/Πλήρως αμφίδρομη"
100Mb-Half-Duplex        = "100Mbps/Ημι-αμφίδρομη"
100Mb-Full-Duplex        = "100Mbps/Πλήρως αμφίδρομη"
1000Mb-Full-Duplex       = "1.0Gbps/Πλήρως αμφίδρομη"
NetworkAddress           = "Διεύθυνση δικτύου"
IPChksumOffv4            = "Μείωση φόρτου αθροίσματος ελέγχου IPv4"
TCPChksumOffv4           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv4)"
UDPChksumOffv4           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv6)"
TCPChksumOffv6           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv6)"
UDPChksumOffv6           = "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv6)"
Enabled                  = "Ενεργοποιημένο"
Disabled                 = "Απενεργοποιημένο"
TxEnabled                = "Ενεργοποιημένο Tx"
RxEnabled                = "Ενεργοποιημένο Rx"
RxTxEnabled              = "Ενεργοποιημένο Rx & Tx"
LSOv4                    = "Μείωση φόρτου μεγάλης αποστολής (IPv4)"
LSOv2v4                  = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv4)"
LSOv2v6                  = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv6)"
FlowControl              = "Έλεγχος ροής"
PriorityVLAN             = "Προτεραιότητα & VLAN"
PriorityVLANDisabled     = "Απενεργοποίηση προτεραιότητας & VLAN"
PriorityVLANEnabled      = "Ενεργοποίηση προτεραιότητας & VLAN"
InterruptModeration      = "Διακοπή επόπτευσης"
ReceiveBuffers           = "Προσωρινοί χώροι παραλαβής"
TransmitBuffers          = "Προσωρινοί χώροι μετάδοσης"
AutoDisableGigabit       = "Gigabit αυτόματης απενεργοποίησης"
AutoLinkDownPhyOff       = "PHY αυτόματης απενεργοποίησης"
BatteryRe-Link           = "Επανασύνδεση, Μπαταρία"
AcBatteryRe-Link         = "Επανασύνδεση, Μπαταρία ή AC"
Battery                  = "Ενεργοποίηση, Μπαταρία"
AcBattery                = "Ενεργοποίηση, Μπαταρία ή AC"
JumboFrame               = "Πλαίσιο Jumbo"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Wake-on-LAN τερματισμού"
AutoLinkDownPcieMacOff   = "PCIe αυτόματης απενεργοποίησης"
RSS                      = "Παραλαβή πλευρικής κλιμάκωσης"
AutoCrossoverDet         = "Αυτόματη ανίχνευση τιμής διασταύρωσης"
PriorityEnabled          = "Ενεργοποίηση προτεραιότητας"
VLANEnabled              = "Ενεργοποίηση VLAN"
10MbFirst                = "Πρώτα 10 Mbps"
100MbFirst               = "Πρώτα 100 Mbps"
WolShutdownLinkSpeed     = "Ταχύτητα σύνδεσης τερματισμού & WOL"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Hebrew
[Strings.040D]
Realtek                  = "Realtek"

AutoDetect               = "משא ומתן אוטומטי"
SpeedDuplex              = "מהירות וכיווניות"
10Mb-Half-Duplex         = "10Mbps חד כיווני"
10Mb-Full-Duplex         = "10Mbps דו כיווני"
100Mb-Half-Duplex        = "100Mbps חד כיווני"
100Mb-Full-Duplex        = "100Mbps דו כיווני"
1000Mb-Full-Duplex       = "1000Mbps דו כיווני"
NetworkAddress           = "כתובת רשת"
IPChksumOffv4            = "העברת סיכום ביקורת IPv4"
TCPChksumOffv4           = "העברת סיכום ביקורת IPv4) TCP)"
UDPChksumOffv4           = "העברת סיכום ביקורת IPv4) UDP)"
TCPChksumOffv6           = "העברת סיכום ביקורת IPv6) TCP)"
UDPChksumOffv6           = "העברת סיכום ביקורת IPv6) UDP)"
Enabled                  = "מאופשר"
Disabled                 = "מבוטל"
TxEnabled                = "שידור מאופשר"
RxEnabled                = "קליטה מאופשרת"
RxTxEnabled              = "שידור וקליטה מאופשרים"
LSOv4                    = "העברת שליחה גדולה (IPv4)"
LSOv2v4                  = "העברת שליחה גדולה IPv4) v2)"
LSOv2v6                  = "העברת שליחה גדולה IPv6) v2)"
FlowControl              = "בקרת זרימה"
PriorityVLAN             = "עדיפות ו-VLAN"
PriorityVLANDisabled     = "עדיפות ו-VLAN מבוטלות"
PriorityVLANEnabled      = "עדיפות ו-VLAN מאופשרות"
InterruptModeration      = "צמצום פסיקות"
ReceiveBuffers           = "מאגרי קליטה"
TransmitBuffers          = "מאגרי שידור"
AutoDisableGigabit       = "ביטול אוטומטי של PowerSaving) Gigabit)"
AutoLinkDownPhyOff       = "ביטול אוטומטי של PowerSaving) PHY)"
BatteryRe-Link           = "קישור מחדש, סוללה"
AcBatteryRe-Link         = "קישור מחדש, סוללה או מתח חילופין (AC)"
Battery                  = "מאופשר, סוללה"
AcBattery                = "מאופשר, סוללה או מתח חילופין (AC)"
JumboFrame               = "מסגרת Jumbo"
2KBMTU	                 = "2KB MTU"
3KBMTU	                 = "3KB MTU"
4KBMTU	                 = "4KB MTU"
5KBMTU	                 = "5KB MTU"
6KBMTU	                 = "6KB MTU"
7KBMTU	                 = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "כיבוי Wake-On-Lan"
AutoLinkDownPcieMacOff   = "ביטול אוטומטי של PowerSaving) PCIe)"
RSS                      = "התאמת גודל בצד הקליטה"
AutoCrossoverDet         = "גילוי אוטומטי של חיבור מוצלב"
PriorityEnabled          = "עדיפות מאופשרת"
VLANEnabled              = "VLAN מאופשר"
10MbFirst                = "10Mbps ראשון"
100MbFirst               = "100Mbps ראשון"
WolShutdownLinkSpeed     = "מהירות קישור כיבוי ו-WOL"
NotSpeedDown             = "ללא האטה"
WolCap                   = "יכולות Wake-On-Lan"
None                     = "ללא"
PatternMatch             = "התאמת תבנית"
MagicPacket              = "מנת קסם"
PatternAndMagic          = "התאמת תבנית ומנת קסם"
GreenEthernet            = "ירוקEthernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Hungarian
[Strings.040e]
Realtek                  = "Realtek"

AutoDetect               = "Automatikus sebesség- és duplexitás-felismerés"
SpeedDuplex              = "Sebesség és duplex"
10Mb-Half-Duplex         = "10 Mbps Félduplex"
10Mb-Full-Duplex         = "10 Mbps Teljes duplex"
100Mb-Half-Duplex        = "100 Mbps Mbps Félduplex"
100Mb-Full-Duplex        = "100 Mbps Teljes duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Teljes duplex"
NetworkAddress           = "Hálózati cím"
IPChksumOffv4            = "IPv4 Ellenőrzőösszeg tehermentesítése"
TCPChksumOffv4           = "TCP Ellenőrzőösszeg tehermentesítése (IPv4)"
UDPChksumOffv4           = "UDP Ellenőrzőösszeg tehermentesítése (IPv4)"
TCPChksumOffv6           = "TCP Ellenőrzőösszeg tehermentesítése (IPv6)"
UDPChksumOffv6           = "UDP Ellenőrzőösszeg tehermentesítése (IPv6)"
Enabled                  = "Engedélyezve"
Disabled                 = "Letiltva"
TxEnabled                = "Tx Engedélyezve"
RxEnabled                = "Rx Engedélyezve"
RxTxEnabled              = "Rx és Tx Engedélyezve"
LSOv4                    = "Nagyobb küldemény tehermentesítése (IPv4)"
LSOv2v4                  = "Nagyobb küldemény tehermentesítése v2 (IPv4)"
LSOv2v6                  = "Nagyobb küldemény tehermentesítése v2 (IPv6)"
FlowControl              = "Áramlásszabályozás"
PriorityVLAN             = "Prioritás és VLAN"
PriorityVLANDisabled     = "Prioritás és VLAN letiltva"
PriorityVLANEnabled      = "Prioritás és VLAN engedélyezve"
InterruptModeration      = "Megszakítás visszatartása"
ReceiveBuffers           = "Vételi pufferek"
TransmitBuffers          = "Átviteli pufferek"
AutoDisableGigabit       = "Gigabit automatikus letiltása"
AutoLinkDownPhyOff       = "PHY automatikus letiltása"
BatteryRe-Link           = "Újrakapcsolódás, akkumulátor"
AcBatteryRe-Link         = "Újrakapcsolódás, akkumulátor vagy AC"
Battery                  = "Engedélyezve, akkumulátor"
AcBattery                = "Engedélyezve, akkumulátor vagy AC"
JumboFrame               = "Jumbo Frame (Óriás keret)"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Felélesztés leállítás után hálózaton keresztül"
AutoLinkDownPcieMacOff   = "PCIe automatikus letiltása"
RSS                      = "Vételoldali skálázás"

AutoCrossoverDet         = "Keresztezés automatikus észlelése"
PriorityEnabled          = "Prioritás engedélyezve"
VLANEnabled              = "VLAN engedélyezve"
10MbFirst                = "10 Mbps/Első"
100MbFirst               = "100 Mbps/Első"
WolShutdownLinkSpeed     = "WOL és leállítás kapcsolati sebessége"
NotSpeedDown             = "Nincs lassítás"
WolCap                   = "Hálózaton keresztül történő felélesztéssel kapcsolatos funkciók"
None                     = "Nincs"
PatternMatch             = "Mintaillesztés"
MagicPacket              = "Megfelelő csomag"
PatternAndMagic          = "Mintaillesztés és megfelelő csomag"
GreenEthernet            = "Energiatakarékos Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Italian
[Strings.0410]
Realtek                  = "Realtek"

AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Velocità e duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
NetworkAddress           = "Indirizzo di rete"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Abilitato"
Disabled                 = "Disabilitato"
TxEnabled                = "Tx Abilitata"
RxEnabled                = "Rx Abilitata"
RxTxEnabled              = "Rx & Tx Abilitata"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Controllo flusso"
PriorityVLAN             = "Priorità e VLAN"
PriorityVLANDisabled     = "Priorità e VLAN disabilitata"
PriorityVLANEnabled      = "Priorità e VLAN abilitata"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Ricevi buffer"
TransmitBuffers          = "Trasmetti buffer"
AutoDisableGigabit       = "Disabilitazione automatica gigabit"
AutoLinkDownPhyOff       = "Disabilitazione automatica PHY"
BatteryRe-Link           = "Ricollegamento, batteria"
AcBatteryRe-Link         = "Ricollegamento, batteria o AC"
Battery                  = "Abilitato, batteria"
AcBattery                = "Abilitato, batteria o AC"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Disabilitazione automatica PCIe"
RSS                      = "Ricevi side scaling"
AutoCrossoverDet         = "Rilevamento automatico crossover"
PriorityEnabled          = "Priorità abilitata"
VLANEnabled              = "VLAN abilitata"
10MbFirst                = "Prima 10 Mbps"
100MbFirst               = "Prima 100 Mbps"
WolShutdownLinkSpeed     = "WOL & Shutdown velocità collegamento"
NotSpeedDown             = "Non rallentamento"
WolCap                   = "Funzioni Wake-On-Lan"
None                     = "Nessuno"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match e Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Japanese
[Strings.0411]
Realtek                  = "Realtek"

AutoDetect               = "自動ネゴシエーション"
SpeedDuplex              = "速度とデュプレックス"
10Mb-Half-Duplex         = "10 Mbps ハーフデュプレックス"
10Mb-Full-Duplex         = "10 Mbps フルデュプレックス"
100Mb-Half-Duplex        = "100 Mbps ハーフデュプレックス"
100Mb-Full-Duplex        = "100 Mbps フルデュプレックス"
1000Mb-Full-Duplex       = "1.0 Gbps フルデュプレックス"
NetworkAddress           = "ネットワークアドレス"
IPChksumOffv4            = "IPv4 チェックサムオフロード"
TCPChksumOffv4           = "TCP チェックサムオフロード (IPv4)"
UDPChksumOffv4           = "UDP チェックサムオフロード (IPv4)"
TCPChksumOffv6           = "TCP チェックサムオフロード (IPv6)"
UDPChksumOffv6           = "UDP チェックサムオフロード (IPv6)"
Enabled                  = "有効"
Disabled                 = "無効"
TxEnabled                = "Tx 有効"
RxEnabled                = "Rx 有効"
RxTxEnabled              = "受信と伝送有効"
LSOv4                    = "一括送信オフロード (IPv4)"
LSOv2v4                  = "一括送信オフロード v2 (IPv4)"
LSOv2v6                  = "一括送信オフロード v2 (IPv6)"
FlowControl              = "フローコントロール"
PriorityVLAN             = "優先度およびVLAN"
PriorityVLANDisabled     = "優先度およびVLAN 無効"
PriorityVLANEnabled      = "優先度およびVLAN 有効"
InterruptModeration      = "割込みモデレーション"
ReceiveBuffers           = "受信バッファ"
TransmitBuffers          = "伝送バッファ"
AutoDisableGigabit       = "自動無効ギガビット"
AutoLinkDownPhyOff       = "自動無効PHY"
BatteryRe-Link           = "再リンク、バッテリ"
AcBatteryRe-Link         = "再リンク、バッテリまたはAC"
Battery                  = "有効、バッテリ"
AcBattery                = "有効、バッテリまたはAC"
JumboFrame               = "ジャンボフレーム"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "LAN 上のウェークアップのシャットダウン"
AutoLinkDownPcieMacOff   = "自動無効 PCIe"
RSS                      = "受信側スケーリング"
AutoCrossoverDet         = "自動クロスオーバー検出"
PriorityEnabled          = "優先度有効"
VLANEnabled              = "VLAN 有効"
10MbFirst                = "10 Mbps 優先"
100MbFirst               = "100 Mbps 優先"
WolShutdownLinkSpeed     = "WOL とシャットダウンリンク速度"
NotSpeedDown             = "速度低下ではない"
WolCap                   = "Wake-On-Lan機能"
None                     = "なし"
PatternMatch             = "パターン適合"
MagicPacket              = "マジックパケット"
PatternAndMagic          = "パターン適合とマジックパケット"
GreenEthernet            = "グリーンイーサネット"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Korean
[Strings.0412]
Realtek                  = "Realtek"

AutoDetect               = "자동 교섭"
SpeedDuplex              = "속도 및 이중"
10Mb-Half-Duplex         = "10 Mbps 반이중"
10Mb-Full-Duplex         = "10 Mbps 전이중"
100Mb-Half-Duplex        = "100 Mbps 반이중"
100Mb-Full-Duplex        = "100 Mbps 전이중"
1000Mb-Full-Duplex       = "1.0 Gbps 전이중"
NetworkAddress           = "네트워크 주소"
IPChksumOffv4            = "IPv4 체크섬 오프로드"
TCPChksumOffv4           = "TCP 체크섬 오프로드(IPv4)"
UDPChksumOffv4           = "UDP 체크섬 오프로드(IPv4)"
TCPChksumOffv6           = "TCP 체크섬 오프로드(IPv6)"
UDPChksumOffv6           = "UDP 체크섬 오프로드(IPv6)"
Enabled                  = "사용"
Disabled                 = "사용 안 함"
TxEnabled                = "Tx 사용"
RxEnabled                = "Rx 사용"
RxTxEnabled              = "Rx/Tx 사용"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "흐름 제어"
PriorityVLAN             = "우선 순위 및 VLAN"
PriorityVLANDisabled     = "우선 순위 및 VLAN 사용 안 함"
PriorityVLANEnabled      = "우선 순위 및 VLAN 사용"
InterruptModeration      = "인터럽트 완화"
ReceiveBuffers           = "수신 버퍼"
TransmitBuffers          = "송신 버퍼"
AutoDisableGigabit       = "Gigabit 자동 비활성화(절전)"
AutoLinkDownPhyOff       = "PHY 자동 비활성화(절전)"
BatteryRe-Link           = "다시 연결, 전지"
AcBatteryRe-Link         = "다시 연결, 전지 또는 AC"
Battery                  = "사용, 전지"
AcBattery                = "사용, 전지 또는 AC"
JumboFrame               = "점보 프레임"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "웨이크 온 랜 종료"
AutoLinkDownPcieMacOff   = "PCIe 자동 비활성화(절전)"
RSS                      = "수신측 조정"
AutoCrossoverDet         = "자동 크로스오버 탐지"
PriorityEnabled          = "우선 순위 사용"
VLANEnabled              = "VLAN 사용"
10MbFirst                = "10 Mbps 먼저"
100MbFirst               = "100 Mbps 먼저"
WolShutdownLinkSpeed     = "WOL 및 종료 링크 속도"
NotSpeedDown             = "속도 저하 안 함"
WolCap                   = "WOL 기능"
None                     = "없음"
PatternMatch             = "패턴 매치"
MagicPacket              = "매직 패킷"
PatternAndMagic          = "패턴 매치와 매직 패킷"
GreenEthernet            = "절전형 이더넷"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Norwegian_Bokmal
[Strings.0414]
Realtek                  = "Realtek"

AutoDetect               = "Automatisk forhandling"
SpeedDuplex              = "Hastighet og dupleks"
10Mb-Half-Duplex         = "10Mbps Halv dupleks"
10Mb-Full-Duplex         = "10Mbps Full dupleks"
100Mb-Half-Duplex        = "100Mbps Halv dupleks"
100Mb-Full-Duplex        = "100Mbps Full dupleks"
1000Mb-Full-Duplex       = "1.0Gbps Full dupleks"
NetworkAddress           = "Nettverksadresse"
IPChksumOffv4            = "IPv4 Sjekksum avlastning"
TCPChksumOffv4           = "TCP Sjekksum avlastning (IPv4)"
UDPChksumOffv4           = "UDP Sjekksum avlastning (IPv4)"
TCPChksumOffv6           = "TCP Sjekksum avlastning (Ipv6)"
UDPChksumOffv6           = "UDP Sjekksum avlastning (Ipv6)"
Enabled                  = "Aktivert"
Disabled                 = "Deaktivert"
TxEnabled                = "Tx aktivert"
RxEnabled                = "Rx aktivert"
RxTxEnabled              = "Rx og Tx aktivert"
LSOv4                    = "Stor sending avlastning (IPv4)"
LSOv2v4                  = "Stor sending avlastning v2 (IPv4)"
LSOv2v6                  = "Stor sending avlastning v2 (Ipv6)"
FlowControl              = "Flytkontroll"
PriorityVLAN             = "Prioritet og VLAN"
PriorityVLANDisabled     = "Prioritet og VLAN deaktivert"
PriorityVLANEnabled      = "Prioritet og VLAN aktivert"
InterruptModeration      = "Avbruddsmoderering"
ReceiveBuffers           = "Mottaksbuffere"
TransmitBuffers          = "Sendebuffere"
AutoDisableGigabit       = "Automatisk deaktivere gigabit"
AutoLinkDownPhyOff       = "Automatisk deaktivere PHY"
BatteryRe-Link           = "Ny linje, batteri"
AcBatteryRe-Link         = "Ny linje, batteri eller vekselstrøm"
Battery                  = "Aktivert, batteri"
AcBattery                = "Aktivert, batteri or vekselstrøm"
JumboFrame               = "Jumbo-ramme"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Avslutningsaktivering på nettverk"
AutoLinkDownPcieMacOff   = "Automatisk deaktivere PCIe"
RSS                      = "Mottak sideskalering"
AutoCrossoverDet         = "Automatisk registrering av grenbytte"
PriorityEnabled          = "Prioritet aktivert"
VLANEnabled              = "VLAN aktivert"
10MbFirst                = "10 Mbps Først"
100MbFirst               = "100 Mbps Først"
WolShutdownLinkSpeed     = "WOL og avslutningslinjehastighet"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Grønt Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Polish
[Strings.0415]
Realtek                  = "Realtek"

AutoDetect               = "Automatyczne negocjacje"
SpeedDuplex              = "Szybkość i dupleks"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
NetworkAddress           = "Adres sieciowy"
IPChksumOffv4            = "Suma kontrolna bez obciążenia IPv4"
TCPChksumOffv4           = "Suma kontrolna bez obciążenia TCP (IPv4)"
UDPChksumOffv4           = "Suma kontrolna bez obciążenia UDP (IPv4)"
TCPChksumOffv6           = "Suma kontrolna bez obciążenia TCP (IPv6)"
UDPChksumOffv6           = "Suma kontrolna bez obciążenia UDP (IPv6)"
Enabled                  = "Włączone"
Disabled                 = "Wyłączone"
TxEnabled                = "Włączone Tx"
RxEnabled                = "Włączone Rx"
RxTxEnabled              = "Włączone Rx i Tx"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Sterowanie przepływem"
PriorityVLAN             = "Priorytet i VLAN"
PriorityVLANDisabled     = "Wyłączony Priorytet i VLAN"
PriorityVLANEnabled      = "Włączony Priorytet i VLAN"
InterruptModeration      = "Moderacja przerwania"
ReceiveBuffers           = "Bufory odbioru"
TransmitBuffers          = "Bufory transmisji"
AutoDisableGigabit       = "Automatyczne wyłączanie Gigabit"
AutoLinkDownPhyOff       = "Automatyczne wyłączanie PHY"
BatteryRe-Link           = "Ponowne podłączenie, bateria"
AcBatteryRe-Link         = "Ponowne podłączenie, bateria lub prąd zmienny"
Battery                  = "Włączone, bateria"
AcBattery                = "Włączone, bateria lub prąd zmienny"
JumboFrame               = "Ramka Jumbo"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Zamknięcie Wybudzanie przy uaktywnieniu sieci"
AutoLinkDownPcieMacOff   = "Automatyczne wyłączenie PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Autodetekcja rodzaju połączenia"
PriorityEnabled          = "Włączony priorytet"
VLANEnabled              = "Włączona sieć VLAN"
10MbFirst                = "Najpierw 10 Mbps"
100MbFirst               = "Najpierw 100 Mbps"
WolShutdownLinkSpeed     = "WOL i szybkość zamykania łącza"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Energooszczędny Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Portuguese_Brazilian
[Strings.0416]
Realtek                  = "Realtek"

AutoDetect               = "Auto Negociação"
SpeedDuplex              = "Velocidade & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
NetworkAddress           = "Endereço de Rede"
IPChksumOffv4            = "IPv4 Descarga de Checksum"
TCPChksumOffv4           = "TCP Descarga de Checksum (IPv4)"
UDPChksumOffv4           = "UDP Descarga de Checksum (IPv4)"
TCPChksumOffv6           = "TCP Descarga de Checksum (IPv6)"
UDPChksumOffv6           = "UDP Descarga de Checksum (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Tx Activado"
RxEnabled                = "Rx Activado"
RxTxEnabled              = "Rx & Tx Activados"
LSOv4                    = "Descarga Large Send (IPv4)"
LSOv2v4                  = "Descarga Large Send v2 (IPv4)"
LSOv2v6                  = "Descarga Large Send v2 (IPv6)"
FlowControl              = "Controlo de Fluxo"
PriorityVLAN             = "Prioridade & VLAN"
PriorityVLANDisabled     = "Prioridade & VLAN Desactivados"
PriorityVLANEnabled      = "Prioridade & VLAN Activados"
InterruptModeration      = "Moderação de Interrupção"
ReceiveBuffers           = "Receber Memórias Intermédias"
TransmitBuffers          = "Transmitir Memórias Intermédias"
AutoDisableGigabit       = "Auto Desactivar Gigabit"
AutoLinkDownPhyOff       = "Auto Desactivar PHY"
BatteryRe-Link           = "Re-Ligar, Bateria"
AcBatteryRe-Link         = "Re-Ligar, Bateria ou AC"
Battery                  = "Activado, Bateria"
AcBattery                = "Activado, Bateria ou CA"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Desligar Despertar Aquando de Lan"
AutoLinkDownPcieMacOff   = "Auto Desactivar PCIe"
RSS                      = "Receber Side Scaling"
AutoCrossoverDet         = "Detecção Auto Crossover"
PriorityEnabled          = "Prioridade Activada"
VLANEnabled              = "VLAN Activada"
10MbFirst                = "10 Mbps Primeiro"
100MbFirst               = "100 Mbps Primeiro"
WolShutdownLinkSpeed     = "WOL & Desligar Velocidade Ligação"
NotSpeedDown             = "Não reduzir velocidade"
WolCap                   = "Capacidades Wake-On-Lan"
None                     = "Nenhum"
PatternMatch             = "Correspondência de padrões"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Correspondência de pacotes e Magic Packet"
GreenEthernet            = "Ethernet Verde"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Portuguese_Standard
[Strings.0816]
Realtek                  = "Realtek"

AutoDetect               = "Auto negociação"
SpeedDuplex              = "Velocidade e modo duplex"
10Mb-Half-Duplex         = "10 Mbps modo semi duplex"
10Mb-Full-Duplex         = "10 Mbps modo full-duplex"
100Mb-Half-Duplex        = "100 Mbps modo semi duplex"
100Mb-Full-Duplex        = "100 Mbps modo full-duplex"
1000Mb-Full-Duplex       = "1,0 Gbps modo full-duplex"
NetworkAddress		 = "Endereço de rede"
IPChksumOffv4            = "Soma de verificação offload IPv4"
TCPChksumOffv4           = "Soma de verificação offload TCP (IPv4)"
UDPChksumOffv4           = "Soma de verificação offload UDP (IPv4)"
TCPChksumOffv6           = "Soma de verificação offload TCP (IPv6)"
UDPChksumOffv6           = "Soma de verificação offload UDP (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Transmissão activada"
RxEnabled                = "Recepção activada"
RxTxEnabled              = "Recepção e transmissão activada"
LSOv4                    = "Envio grande de offload (IPv4)"
LSOv2v4                  = "Envio grande de offload v2 (IPv4)"
LSOv2v6                  = "Envio grande de offload v2 (IPv6)"
FlowControl              = "Controlo do fluxo"
PriorityVLAN             = "Prioridade e VLAN"
PriorityVLANDisabled     = "Prioridade e VLAN desactivada"
PriorityVLANEnabled      = "Prioridade e VLAN activada"
InterruptModeration      = "Moderação de interrupção"
ReceiveBuffers           = "Memória de recepção"
TransmitBuffers          = "Memória de transmissão"
AutoDisableGigabit       = "Desactivar Gigabit automaticamente"
AutoLinkDownPhyOff       = "Desactivar PHY automaticamente"
BatteryRe-Link           = "Religar, bateria"
AcBatteryRe-Link         = "Religar, bateria ou a.c."
Battery                  = "Activada, bateria"
AcBattery                = "Activada, bateria ou a.c."
JumboFrame               = "Estrutura jumbo"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Encerrar Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Desactivar PCIe automaticamente"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Detecção cruzada automática"
PriorityEnabled          = "Prioridade activada"
VLANEnabled              = "VLAN activada"
10MbFirst                = "10 Mbps primeiro"
100MbFirst               = "100 Mbps primeiro"
WolShutdownLinkSpeed     = "WOL e encerrar velocidade de ligação"
NotSpeedDown             = "Não diminuir velocidade"
WolCap                   = "Capacidades Wake-On-Lan"
None                     = "Nenhuma"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match e Magic Packet"
GreenEthernet            = "Ethernet verde"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Romanian
[Strings.0418]
Realtek                  = "Realtek"
AutoDetect               = "Negociere automată"
SpeedDuplex              = "Viteză şi duplex"
10Mb-Half-Duplex         = "10 Mbps semiduplex"
10Mb-Full-Duplex         = "10 Mbps duplex"
100Mb-Half-Duplex        = "100 Mbps semiduplex"
100Mb-Full-Duplex        = "100 Mbps duplex"
1000Mb-Full-Duplex       = "1,0 Gbps duplex"
NetworkAddress		 = "Adresă de reţea"
IPChksumOffv4            = "Preluare sarcină de verificare erori de transmisie IPv4"
TCPChksumOffv4           = "Preluare sarcină de verificare erori de transmisie TCP (IPv4)"
UDPChksumOffv4           = "Preluare sarcină de verificare erori de transmisie UDP(IPv4)"
TCPChksumOffv6           = "Preluare sarcină de verificare erori de transmisie TCP(IPv6)"
UDPChksumOffv6           = "Preluare sarcină de verificare erori de transmisie UDP (IPv6)"
Enabled                  = "Activat"
Disabled                 = "Dezactivat"
TxEnabled                = "Tx activat"
RxEnabled                = "Rx activat"
RxTxEnabled              = "Rx şi Tx activate"
LSOv4                    = "Preluare sarcină de trimitere pachete mari(IPv4)"
LSOv2v4                  = "Preluare sarcină de trimitere pachete mari v2 (IPv4)"
LSOv2v6                  = "Preluare sarcină de trimitere pachete mari v2 (IPv6)"
FlowControl              = "Control debit"
PriorityVLAN             = "Prioritate şi VLAN"
PriorityVLANDisabled     = "Prioritate şi VLAN dezactivate"
PriorityVLANEnabled      = "Prioritate şi VLAN activate"
InterruptModeration      = "Moderare întrerupere"
ReceiveBuffers           = "Zone tampon de primire"
TransmitBuffers          = "Zone tampon de trimitere"
AutoDisableGigabit       = "Dezactivare automată Gigabit"
AutoLinkDownPhyOff       = "Dezactivare automată PHY"
BatteryRe-Link           = "Reconectare, baterie"
AcBatteryRe-Link         = "Reconectare, baterie sau AC"
Battery                  = "Activat, baterie"
AcBattery                = "Activat, baterie sau AC"
JumboFrame               = "Cadru jumbo"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Închidere Trezire prin LAN"
AutoLinkDownPcieMacOff   = "Dezactivare automată PCIe"
RSS                      = "Primire scalare laterală"
AutoCrossoverDet         = "Detectare automată simulare modem"
PriorityEnabled          = "Prioritate activată"
VLANEnabled              = "VLAN activată"
10MbFirst                = "10 Mbps iniţial"
100MbFirst               = "100 Mbps iniţial"
WolShutdownLinkSpeed     = "WOL şi dezactivare viteză legătură"
NotSpeedDown             = "Fără reducere viteză"
WolCap                   = "Capacităţi trezire prin LAN"
None                     = "Niciun(a)"
PatternMatch             = "Potrivire obiecte"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Potrivire pachete şi Magic Packet"
GreenEthernet            = "Ethernet verde"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Russian
[Strings.0419]
Realtek                  = "Realtek"

AutoDetect               = "Автосогласование"
SpeedDuplex              = "Скорость и дуплекс"
10Mb-Half-Duplex         = "10 Мбит/с полудуплекс"
10Mb-Full-Duplex         = "10 Мбит/с дуплекс"
100Mb-Half-Duplex        = "100 Мбит/с полудуплекс"
100Mb-Full-Duplex        = "100 Мбит/с дуплекс"
1000Mb-Full-Duplex       = "1 Гбит/с дуплекс"
NetworkAddress		 = "Сетевой адрес"
IPChksumOffv4            = "Контрольная сумма разгрузки IPv4"
TCPChksumOffv4           = "Контрольная сумма разгрузки TCP (IPv4)"
UDPChksumOffv4           = "Контрольная сумма разгрузки UDP (IPv4)"
TCPChksumOffv6           = "Контрольная сумма разгрузки TCP (IPv6)"
UDPChksumOffv6           = "Контрольная сумма разгрузки UDP (IPv6)"
Enabled                  = "Вкл"
Disabled                 = "Выкл"
TxEnabled                = "Tx вкл"
RxEnabled                = "Rx вкл"
RxTxEnabled              = "Rx & Tx вкл"
LSOv4                    = "Разгрузка при большой отправке (IPv4)"
LSOv2v4                  = "Разгрузка при большой отправке v2 (IPv4)"
LSOv2v6                  = "Разгрузка при большой отправке v2 (IPv6)"
FlowControl              = "Управление потоком"
PriorityVLAN             = "Приоритет & VLAN"
PriorityVLANDisabled     = "Приоритет & VLAN выкл"
PriorityVLANEnabled      = "Приоритет & VLAN вкл"
InterruptModeration      = "Модерация прерывания"
ReceiveBuffers           = "Буферы приема"
TransmitBuffers          = "Буферы передачи"
AutoDisableGigabit       = "Автоотключение гигабитной скорости"
AutoLinkDownPhyOff       = "Автоотключение PHY"
BatteryRe-Link           = "Переподключение, батарея"
AcBatteryRe-Link         = "Переподключение, батарея или пер. ток"
Battery                  = "Вкл, батарея"
AcBattery                = "Вкл, батарея или пер. ток"
JumboFrame               = "Большой кадр"
2KBMTU                   = "2KБ MTU"
3KBMTU                   = "3KБ MTU"
4KBMTU                   = "4KБ MTU"
5KBMTU                   = "5KБ MTU"
6KBMTU                   = "6KБ MTU"
7KBMTU                   = "7KБ MTU"
8KBMTU                   = "8KБ MTU"
9KBMTU                   = "9KБ MTU"
S5WakeOnLan              = "Включение по локальной сети после отключения"
AutoLinkDownPcieMacOff   = "Автоотключение PCIe"
RSS                      = "Получение бокового масштабирования"
AutoCrossoverDet         = "Автоопределение кросс-кабеля"
PriorityEnabled          = "Приоритет вкл"
VLANEnabled              = "VLAN вкл"
10MbFirst                = "Сначала 10 Mбит/с"
100MbFirst               = "Сначала 100 Mбит/с"
WolShutdownLinkSpeed     = "Скорость при включении по локальной сети после отключения"
NotSpeedDown             = "Не использовать автопонижение скорости"
WolCap                   = "Функции включения по сети"
None                     = "Нет"
PatternMatch             = "Соответствие шаблону"
MagicPacket              = "Специальный пакет"
PatternAndMagic          = "Соответствие шаблону И Специальный пакет"
GreenEthernet            = "Зеленый Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Slovak
[Strings.041b]
Realtek                  = "Realtek"
AutoDetect               = "Automatické vyjednávanie"
SpeedDuplex              = "Rýchlosť a duplexný režim"
10Mb-Half-Duplex         = "10 Mbps polovične duplexný"
10Mb-Full-Duplex         = "10 Mbps plne duplexný"
100Mb-Half-Duplex        = "100 Mbps polovične duplexný"
100Mb-Full-Duplex        = "100 Mbps plne duplexný"
1000Mb-Full-Duplex       = "1,0 Gbps plne duplexný"
NetworkAddress		 = "Sieťová adresa"
IPChksumOffv4            = "Kontrolný súčet zníženej záťaže IPv4"
TCPChksumOffv4           = "Kontrolný súčet zníženej záťaže TCP (IPv4)"
UDPChksumOffv4           = "Kontrolný súčet zníženej záťaže UDP (IPv4)"
TCPChksumOffv6           = "Kontrolný súčet zníženej záťaže TCP (IPv6)"
UDPChksumOffv6           = "Kontrolný súčet zníženej záťaže UDP (IPv6)"
Enabled                  = "Aktivovaný"
Disabled                 = "Deaktivovaný"
TxEnabled                = "Tx aktivovaný"
RxEnabled                = "Rx aktivovaný"
RxTxEnabled              = "Rx a Tx aktivované"
LSOv4                    = "Veľká odoslaná znížená záťaž (IPv4)"
LSOv2v4                  = "Veľká odoslaná znížená záťaž v2 (IPv4)"
LSOv2v6                  = "Veľká odoslaná znížená záťaž v2 (IPv6)"
FlowControl              = "Ovládanie toku"
PriorityVLAN             = "Priorita a VLAN"
PriorityVLANDisabled     = "Priorita a VLAN sú deaktivované"
PriorityVLANEnabled      = "Priorita a VLAN sú aktivované"
InterruptModeration      = "Prerušiť moderovanie"
ReceiveBuffers           = "Medzipamäte pre príjem"
TransmitBuffers          = "Medzipamäte pre prenos"
AutoDisableGigabit       = "Automaticky zablokovať Gigabit"
AutoLinkDownPhyOff       = "Automaticky zablokovať PHY"
BatteryRe-Link           = "Opätovne spojiť, batéria"
AcBatteryRe-Link         = "Opätovne spojiť, batéria alebo striedavý prúd"
Battery                  = "Aktivovaný, batéria"
AcBattery                = "Aktivovaný, batéria alebo striedavý prúd"
JumboFrame               = "Jumbo rámček"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Vypnutie po pripojení k LAN"
AutoLinkDownPcieMacOff   = "Automaticky zablokovať PCIe"
RSS                      = "Prijať bočnú zmenu mierky"
AutoCrossoverDet         = "Automatické zistenie hraničnej hodnoty"
PriorityEnabled          = "Priorita je aktivovaná"
VLANEnabled              = "VLAN je aktivovaná"
10MbFirst                = "Najprv 10 Mbps"
100MbFirst               = "Najprv 100 Mbps"
WolShutdownLinkSpeed     = "Rýchlosť WOL a vypnutia spojenia"
NotSpeedDown             = "Neznížiť rýchlosť"
WolCap                   = "Možnosti po pripojení k LAN"
None                     = "Žiadne"
PatternMatch             = "Zhoda vzorky"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Zhoda vzorky a Magic Packet"
GreenEthernet            = "Zelený Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Slovenian
[Strings.0424]
Realtek                  = "Realtek"

AutoDetect               = "Samopogajanje"
SpeedDuplex              = "Hitrost in dupleks"
10Mb-Half-Duplex         = "10 Mb/s Polovični dupleks"
10Mb-Full-Duplex         = "10 Mb/s Polni dupleks"
100Mb-Half-Duplex        = "100 Mb/s Polovični dupleks"
100Mb-Full-Duplex        = "100 Mb/s Polni dupleks"
1000Mb-Full-Duplex       = "1.0 Gb/s Polni dupleks"
NetworkAddress           = "Omrežni naslov"
IPChksumOffv4            = "IPv4 Razbremenitev kontrolne vsote"
TCPChksumOffv4           = "TCP Razbremenitev kontrolne vsote (IPv4)"
UDPChksumOffv4           = "UDP Razbremenitev kontrolne vsote (IPv4)"
TCPChksumOffv6           = "TCP Razbremenitev kontrolne vsote (IPv6)"
UDPChksumOffv6           = "UDP Razbremenitev kontrolne vsote (IPv6)"
Enabled                  = "Omogočeno"
Disabled                 = "Onemogočeno"
TxEnabled                = "Tx Omogočeno"
RxEnabled                = "Rx Omogočeno"
RxTxEnabled              = "Rx in Tx omogočeno"
LSOv4                    = "Razbremenitev velikega prenosa (IPv4)"
LSOv2v4                  = "Razbremenitev velikega prenosa v2 (IPv4)"
LSOv2v6                  = "Razbremenitev velikega prenosa v2 (IPv6)"
FlowControl              = "Kontrola pretoka"
PriorityVLAN             = "Prednost in VLAN"
PriorityVLANDisabled     = "Prednost in VLAN onemogočena"
PriorityVLANEnabled      = "Prednost in VLAN omogočena"
InterruptModeration      = "Prekinjena moderacija"
ReceiveBuffers           = "Prejmi medpomnilnike"
TransmitBuffers          = "Prenesi medpomnilnike"
AutoDisableGigabit       = "Samodejno onemogočenje Gigabit"
AutoLinkDownPhyOff       = "Samodejno onemogočenje PHY"
BatteryRe-Link           = "Po-povezava, baterija"
AcBatteryRe-Link         = "Po-povezava, baterija ali AC"
Battery                  = "Omogočeno, baterija"
AcBattery                = "Omogočeno, baterija ali AC"
JumboFrame               = "Jumbo okvir"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Zaustavitev Bujenje-na-Lan"
AutoLinkDownPcieMacOff   = "Samodejno onemogočenje PCIe"
RSS                      = "Sprejmi stransko merilo"
AutoCrossoverDet         = "Samodejno križno zaznavanje"
PriorityEnabled          = "Prednost omogočena"
VLANEnabled              = "VLAN omogočen"
10MbFirst                = "10 Mb/s Najprej"
100MbFirst               = "100 Mb/s Najprej"
WolShutdownLinkSpeed     = "Hitrost zaustavitve povezave in WOL"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Zeleni Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Spanish
[Strings.040A]
Realtek                  = "Realtek"

AutoDetect               = "Negociación automática"
SpeedDuplex              = "Velocidad y Dúplex"
10Mb-Half-Duplex         = "10 Mbps Half Dúplex"
10Mb-Full-Duplex         = "10 Mbps Full Dúplex"
100Mb-Half-Duplex        = "100 Mbps Half Dúplex"
100Mb-Full-Duplex        = "100 Mbps Full Dúplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Dúplex"
NetworkAddress           = "Dirección de red"
IPChksumOffv4            = "Descarga de suma de comprobación IPv4"
TCPChksumOffv4           = "Descarga de suma de comprobación TCP (IPv4)"
UDPChksumOffv4           = "Descarga de suma de comprobación UDP (IPv4)"
TCPChksumOffv6           = "Descarga de suma de comprobación TCP (IPv6)"
UDPChksumOffv6           = "Descarga de suma de comprobación UDP (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Tx activada"
RxEnabled                = "Rx activada"
RxTxEnabled              = "Rx y Tx activado"
LSOv4                    = "Descarga de gran envío (IPv4)"
LSOv2v4                  = "Descarga de gran envío v2 (IPv4)"
LSOv2v6                  = "Descarga de gran envío v2 (IPv6)"
FlowControl              = "Control de flujo"
PriorityVLAN             = "Prioridad y VLAN"
PriorityVLANDisabled     = "Prioridad y VLAN desactivada"
PriorityVLANEnabled      = "Prioridad y VLAN activada"
InterruptModeration      = "Moderación de interrupción"
ReceiveBuffers           = "Búferes de recepción"
TransmitBuffers          = "Búferes de transmisión"
AutoDisableGigabit       = "Desactivar Gigabit automáticamente"
AutoLinkDownPhyOff       = "Desactivar PHY automáticamente"
BatteryRe-Link           = "Reenlazar, batería"
AcBatteryRe-Link         = "Reenlazar, batería o AC"
Battery                  = "Activado, batería"
AcBattery                = "Activado, batería o AC"
JumboFrame               = "Trama Jumbo"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Activación con LAN de apagado"
AutoLinkDownPcieMacOff   = "Desactivar automáticamente PCIe"
RSS                      = "Escalado lateral de recepción"
AutoCrossoverDet         = "Detección automática de cruce"
PriorityEnabled          = "Prioridad habilitada"
VLANEnabled              = "VLAN activada"
10MbFirst                = "10 Mbps Primero"
100MbFirst               = "100 Mbps Primero"
WolShutdownLinkSpeed     = "Velocidad de enlace WOL y Apagado"
NotSpeedDown             = "Sin reducción de velocidad"
WolCap                   = "Funciones Wake-On-Lan"
None                     = "Ninguno"
PatternMatch             = "Comparar patrón"
MagicPacket              = "Paquete mágico"
PatternAndMagic          = "Comparar patrón y paquete mágico"
GreenEthernet            = "Ethernet ecológico"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Swedish
[Strings.041D]
Realtek                  = "Realtek"


AutoDetect               = "Automatisk förhandling"
SpeedDuplex              = "Hastighet & duplex"
10Mb-Half-Duplex         = "10 Mbps Halv duplex"
10Mb-Full-Duplex         = "10 Mbps Full duplex"
100Mb-Half-Duplex        = "100 Mbps Halv duplex"
100Mb-Full-Duplex        = "100 Mbps Full duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full duplex"
NetworkAddress           = "Nätverksadress"
IPChksumOffv4            = "IPv4 Avbelasta kontrollsumma"
TCPChksumOffv4           = "TCP avbelasta kontrollsumma (IPv4)"
UDPChksumOffv4           = "UDP avbelasta kontrollsumma (IPv4)"
TCPChksumOffv6           = "TCP avbelasta kontrollsumma (IPv6)"
UDPChksumOffv6           = "UDP avbelasta kontrollsumma (IPv6)"
Enabled                  = "Aktiverad"
Disabled                 = "Inaktiverad"
TxEnabled                = "Tx aktiverad"
RxEnabled                = "Rx aktiverad"
RxTxEnabled              = "Rx & Tx aktiverad"
LSOv4                    = "Avbelastning för stor överföring (IPv4)"
LSOv2v4                  = "Avbelastning för stor överföring v2 (IPv4)"
LSOv2v6                  = "Avbelastning för stor överföring v2 (IPv6)"
FlowControl              = "Flödeskontroll"
PriorityVLAN             = "Prioritet & VLAN"
PriorityVLANDisabled     = "Prioritet & VLAN inaktiverad"
PriorityVLANEnabled      = "Prioritet & VLAN aktiverad"
InterruptModeration      = "Gruppering av avbrott"
ReceiveBuffers           = "Mottagningsbuffertar"
TransmitBuffers          = "Överföringsbuffertar"
AutoDisableGigabit       = "Automatisk inaktivering av gigabit"
AutoLinkDownPhyOff       = "Automatisk inaktivering av PHY"
BatteryRe-Link           = "Länka om, batteri"
AcBatteryRe-Link         = "Länka om, batteri eller AC"
Battery                  = "Aktiverad, batteri"
AcBattery                = "Aktiverad, batteri eller AC"
JumboFrame               = "Jumboram"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Avsluta Wake-on-LAN"
AutoLinkDownPcieMacOff   = "Automatisk inaktivering av PCIe"
RSS                      = "Ta emot sidskalning"
AutoCrossoverDet         = "Automatisk crossover-identifiering"
PriorityEnabled          = "Prioritet aktiverad"
VLANEnabled              = "VLAN aktiverat"
10MbFirst                = "10 Mbps först"
100MbFirst               = "100 Mbps först"
WolShutdownLinkSpeed     = "WOL och länkhastighet vid avslutning"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Grönt Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Thai
[Strings.041E]
Realtek                  = "Realtek"

AutoDetect               = "การปรับอัตโนมัติ"
SpeedDuplex              = "ความเร็ว & ดูเพล็กซ์"
10Mb-Half-Duplex         = "10 Mbps ฮาล์ฟดูเพล็กซ์"
10Mb-Full-Duplex         = "10 Mbps ฟุลดูเพล็กซ์"
100Mb-Half-Duplex        = "100 Mbps ฮาล์ฟดูเพล็กซ์"
100Mb-Full-Duplex        = "100 Mbps ฟุลดูเพล็กซ์"
1000Mb-Full-Duplex       = "1.0 Gbps ฟุลดูเพล็กซ์"
NetworkAddress		 =	 "เน็ตเวิร์กแอดเดรส"
IPChksumOffv4            = "IPv4 เช็คซัม ออฟโหลด"
TCPChksumOffv4           = "TCP เช็คซัม ออฟโหลด (IPv4)"
UDPChksumOffv4           = "UDP เช็คซัม ออฟโหลด (IPv4)"
TCPChksumOffv6           = "TCP เช็คซัม ออฟโหลด (IPv6)"
UDPChksumOffv6           = "UDP เช็คซัม ออฟโหลด (IPv6)"
Enabled                  = "เปิดทำงาน"
Disabled                 = "ปิดทำงาน"
TxEnabled                = "Tx เปิดทำงาน"
RxEnabled                = "Rx เปิดทำงาน"
RxTxEnabled              = "Rx & Tx เปิดทำงาน"
LSOv4                    = "ส่งออฟโหลดขนาดใหญ่ (IPv4)"
LSOv2v4                  = "ส่งออฟโหลดขนาดใหญ่ v2 (IPv4)"
LSOv2v6                  = "ส่งออฟโหลดขนาดใหญ่ v2 (IPv6)"
FlowControl              = "โฟลว์คอนโทรล"
PriorityVLAN             = "ลำดับความสำคัญ & VLAN "
PriorityVLANDisabled     = "ลำดับความสำคัญ & VLAN ปิดทำงาน"
PriorityVLANEnabled      = "ลำดับความสำคัญ & VLAN เปิดทำงาน"
InterruptModeration      = "ขัดจังหวะโมเดอเรชัน"
ReceiveBuffers           = "บัฟเฟอร์รับ"
TransmitBuffers          = "บัฟเฟอร์รับส่ง"
AutoDisableGigabit       = "ปิดทำงานกิกะบิตอัตโนมัติ"
AutoLinkDownPhyOff       = "ปิดทำงาน PHY อัตโนมัติ"
BatteryRe-Link           = "ลิงค์ใหม่, แบตเตอรี่"
AcBatteryRe-Link         = "ลิงค์ใหม่, แบตเตอรี่หรือ AC"
Battery                  = "เปิดทำงาน, แบตเตอรี่"
AcBattery                = "เปิดทำงาน, แบตเตอรี่หรือ AC"
JumboFrame               = "จัมโบ เฟรม"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "การปลุกแลนหลังปิดเครื่อง"
AutoLinkDownPcieMacOff   = "ปิดทำงาน PCIe อัตโนมัติ"
RSS                      = "การเปลี่ยนขนาดด้านที่ได้รับ"
AutoCrossoverDet         = "การตรวจจับครอสโอเวอร์อัตโนมัติ"
PriorityEnabled          = "ลำดับความสำคัญเปิดทำงาน"
VLANEnabled              = "VLAN เปิดทำงาน"
10MbFirst                = "10 Mbps ก่อน"
100MbFirst               = "100 Mbps ก่อน"
WolShutdownLinkSpeed     = "ความเร็วลิงค์การปลุกแลน & ปิดเครื่อง"
NotSpeedDown             = "ไม่ลดความเร็ว"
WolCap                   = "คุณสมบัติการปลุกแลน"
None                     = "ไม่มี"
PatternMatch             = "รูปแบบตรง"
MagicPacket              = "เมจิก แพคเก็ต"
PatternAndMagic          = "รูปแบบตรง & เมจิก แพคเก็ต"
GreenEthernet            = "กรีนอีเธอร์เน็ต"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Turkish
[Strings.041F]
Realtek                  = "Realtek"

AutoDetect               = "Otomatik Görüşme"
SpeedDuplex              = "Hız & İkili"
10Mb-Half-Duplex         = "10 Mbps Yarım İkili"
10Mb-Full-Duplex         = "10 Mbps Tam İkili"
100Mb-Half-Duplex        = "100 Mbps Yarım İkili"
100Mb-Full-Duplex        = "100 Mbps Tam İkili"
1000Mb-Full-Duplex       = "1.0 Gbps Tam İkili"
NetworkAddress           = "Ağ Adresi"
IPChksumOffv4            = "IPv4 Boşaltmayı Sağla"
TCPChksumOffv4           = "TCP Boşaltmayı Sağla (IPv4)"
UDPChksumOffv4           = "UDP Boşaltmayı Sağla (IPv4)"
TCPChksumOffv6           = "TCP Boşaltmayı Sağla (IPv6)"
UDPChksumOffv6           = "UDP Boşaltmayı Sağla (IPv6)"
Enabled                  = "Etkinleştirildi"
Disabled                 = "Devre Dışı Bırakıldı"
TxEnabled                = "Tx Etkinleştirildi"
RxEnabled                = "Rx Etkinleştirildi"
RxTxEnabled              = "Rx & Tx Etkinleştirildi"
LSOv4                    = "Boşaltmayı Geniş Gönder (IPv4)"
LSOv2v4                  = "Boşaltmayı Geniş Gönder v2 (IPv4)"
LSOv2v6                  = "Boşaltmayı Geniş Gönder v2 (IPv6)"
FlowControl              = "Akış Denetimi"
PriorityVLAN             = "Öncelik & VLAN"
PriorityVLANDisabled     = "Öncelik & VLAN Devre Dışı Bırakıldı"
PriorityVLANEnabled      = "Öncelik & VLAN Etkinleştirildi"
InterruptModeration      = "Hafifletmeyi Kes"
ReceiveBuffers           = "Arabellekleri Al"
TransmitBuffers          = "Arabellekleri İlet"
AutoDisableGigabit       = "Gigabit’i (PowerSaving) Otomatik Olarak Devredışı Bırak"
AutoLinkDownPhyOff       = "PHY’yi (PowerSaving) Otomatik Olarak Devredışı Bırak"
BatteryRe-Link           = "Yeniden Bağla, Pil"
AcBatteryRe-Link         = "Yeniden Bağla, Pil veya AC"
Battery                  = "Etkinleştirildi, Pil"
AcBattery                = "Etkinleştirildi, Pil veya AC"
JumboFrame               = "Jumbo Çerçeve"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Yerel Ağ Üzerinden Kapat"
AutoLinkDownPcieMacOff   = "PCIe’yi (PowerSaving) Otomatik Olarak Devredışı Bırak"
RSS                      = "Yan Ölçüyü Al"
AutoCrossoverDet         = "Otomatik Geçiş Algılama"
PriorityEnabled          = "Öncelik Etkinleştirildi"
VLANEnabled              = "VLAN Etkinleştirildi"
10MbFirst                = "10 Mbps Önce"
100MbFirst               = "100 Mbps Önce"
WolShutdownLinkSpeed     = "WOL & Kapatma Bağlantı Hızı"
NotSpeedDown             = "Yavaşlatma Değil"
WolCap                   = "Lan’da Uyan Özellikleri"
None                     = "Yok"
PatternMatch             = "Örnek Eşleşmesi"
MagicPacket              = "Sihirli Paket"
PatternAndMagic          = "Örnek Eşleşmesi & Sihirli Paket"
GreenEthernet            = "Yeşil Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"

rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

; Vietnamese
[Strings.042A]
Realtek                  = "Realtek"

AutoDetect               = "Tự động thỏa thuận"
SpeedDuplex              = "Tốc độ & Song công"
10Mb-Half-Duplex         = "10 Mb/giây bán song công"
10Mb-Full-Duplex         = "10 Mb/giây song công hoàn toàn"
100Mb-Half-Duplex        = "100 Mb/giây bán song công"
100Mb-Full-Duplex        = "100 Mb/giây song công hoàn toàn"
1000Mb-Full-Duplex       = "1 Gb/giây song công hoàn toàn"
NetworkAddress		 = "Địa chỉ mạng"
IPChksumOffv4            = "Tải kiểm tra tổng IPv4"
TCPChksumOffv4           = "Tải kiểm tra tổng TCP (IPv4)"
UDPChksumOffv4           = "Tải kiểm tra tổng UDP (IPv4)"
TCPChksumOffv6           = "Tải kiểm tra tổng TCP (IPv6)"
UDPChksumOffv6           = "Tải kiểm tra tổng UDP (IPv6)"
Enabled                  = "Bật"
Disabled                 = "Tắt"
TxEnabled                = "Tx bật"
RxEnabled                = "Rx bật"
RxTxEnabled              = "Rx & Tx bật"
LSOv4                    = "Tải nội dung lớn (IPv4)"
LSOv2v4                  = "Tải nội dung lớn v2 (IPv4)"
LSOv2v6                  = "Tải nội dung lớn v2 (IPv6)"
FlowControl              = "Kiểm soát lưu lượng"
PriorityVLAN             = "Ưu tiên & VLAN"
PriorityVLANDisabled     = "Ưu tiên & VLAN tắt"
PriorityVLANEnabled      = "Ưu tiên & VLAN bật"
InterruptModeration      = "Ngắt kiểm soát"
ReceiveBuffers           = "Bộ nhớ đệm nhận"
TransmitBuffers          = "Bộ nhớ đệm gửi"
AutoDisableGigabit       = "Tự động tắt Gigabit (Tiết kiệm năng lượng)"
AutoLinkDownPhyOff       = "Tự động tắt PHY (Tiết kiệm năng lượng)"
BatteryRe-Link           = "Kết nối lại pin"
AcBatteryRe-Link         = "Kết nối lại pin hoặc AC"
Battery                  = "Pin bật"
AcBattery                = "Pin hoặc AC bật"
JumboFrame               = "Khung mở rộng"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "LAN hiện hành khi tắt máy"
AutoLinkDownPcieMacOff   = "Tự động tắt PCIe (Tiết kiệm năng lượng)"
RSS                      = "Tỷ lệ bên nhận"
AutoCrossoverDet         = "Tự động bỏ dò tìm"
PriorityEnabled          = "Ưu tiên bật"
VLANEnabled              = "VLAN bật"
10MbFirst                = "10 Mb/giây trước"
100MbFirst               = "100 Mb/giây trước"
WolShutdownLinkSpeed     = "LAN hiện hành & Tắt tốc độ kết nối"
NotSpeedDown             = "Không giảm tốc độ"
WolCap                   = "Chức năng LAN hiện hành"
None                     = "Không áp dụng"
PatternMatch             = "Khớp kiểu"
MagicPacket              = "Gói ảo"
PatternAndMagic          = "Khớp kiểu & Gói ảo"
GreenEthernet            = "Ethernet xanh"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy Efficient Ethernet"
HDSplit                  = "Header Data Split"

RTL8169.DeviceDesc       = "Realtek PCI GBE Family Controller"
R8169C7k.DeviceDesc      = "Realtek PCI GBE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8136HP.DeviceDesc     = "Realtek PCIe FE Family Controller"
RTL8168C.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc     = "Realtek PCIe GBE Family Controller"
RTL8168E.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8168F.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8102.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8105.DeviceDesc       = "Realtek PCIe FE Family Controller"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"


rtl8167.Service.DispName = "Realtek 8167 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"

;;;;; InfVer = 2.000