Marvell Yukon Gigabit Ethernet Drivers INSTALLATION(For Windows XP 64bit)

1. Open 'Device Manager'.

2. Open the properties for the 'Marvell Yukon 88E8053 PCI-E Gigabit Ethernet controller'.

3. Select 'Update Driver'.

4. Point the installer to the folder with the '\LAN\Marvell'.

5. It should select the 'Yk51x86.inf' and then install the system files.