InS_StArT
SIS190.COM
1.0
^SiS 191/190 PCI Gigabit Ethernet,SIS190.COM,0E0
?This driver supports PCI machines
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!O0E0(Mediatype)Media Access Type
?NOTE: Media access type will be autodetected on driver's load
UTP
UTPFULL
FAST
FASTFULL
@AUTO
InS_EnD
