There are two protocol boot rom supported. PXE and RPL protocol.

Download remote boot win95 document and driver from
   ftp://210.192.0.122/lancard/information/rpl.exe
   
Download your RPL rom ,"rpl-8139(314).exe" from
   ftp://210.192.0.122/lancard/drivers/8139/rpl-8139(314).exe

Download your PXE/RPL merged rom ,"pxe-rpl(210).exe" from
   ftp://210.192.0.122/lancard/drivers/8139/pxe-rpl(210).exe
		
Download your Flash ROM utility tool ,"rtflash130.exe" from
   ftp://210.192.0.122/lancard/drivers/8139/rtflash(150)-8139.exe

Technical Support or More Information	 
Contact to:	cnfae@realtek.com.tw
 		TEL: 886-3-5780211 Ext 3858/3809 [Jack]
 
