;; NETRTS5.INF (NT 5.x & Win98 combined inf for NDIS5 driver)
;;
;; Realtek RTL8139-Based Fast Ethernet Network Interface Cards.
;;
;; Copyright 2001, Realtek Semiconductor Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature   = "$Chicago$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%                               ;;
CatalogFile = netrts.cat                              ;; for WHQL certified
CatalogFile.NT = netrts2k.cat
DriverVer   = 12/31/2001,5.502.1231.2001

[Manufacturer]
%Realtek%   = Realtek

[ControlFlags]
ExcludeFromSelect = PCI\VEN_10EC&DEV_8139

[Realtek]
; DisplayName            Section        DeviceID
; -----------            -------        --------
%RTL8139.DeviceDesc%   = RTL8139.ndi,   PCI\VEN_10EC&DEV_8139
%RTL8139P.DeviceDesc%  = RTL8139P.ndi,  PCI\VEN_10EC&DEV_8139&REV_20
;%RTL8139.DeviceDesc%   = RTL8139.ndi,   PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC
;%RTL8139P.DeviceDesc%  = RTL8139P.ndi,  PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20

;;****************************************************************************
;; Windows 9x
;;****************************************************************************
;----------------
; RTL8139 Family
;----------------
[rtl8139.ndi]
DriverVer       = 12/31/2001,502
AddReg          = rtl8139.id.reg, RTL8139.common.reg, RTL8139.win.reg
CopyFiles       = RTL8139.CopyFiles98
;DeviceID        = "PCI\VEN_10EC&DEV_8139"
;LogConfig       = DefaultConfig

;------------
; RTL8139c +
;------------
[rtl8139P.ndi]
DriverVer       = 12/31/2001,502
AddReg          = rtl8139.id.reg, RTL8139P.common.reg, RTL8139.win.reg
CopyFiles       = RTL8139.CopyFiles98
;DeviceID        = "PCI\VEN_10EC&DEV_8139"
;LogConfig       = DefaultConfig

;;****************************************************************************
;; NT 5.x
;;****************************************************************************
;----------------
; RTL8139 Family
;----------------
[RTL8139.ndi.NT]
AddReg          = RTL8139.common.reg, RTL8139.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8139.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = rtl8139, 2, rtsnt.Service, RTL8139.EventLog

;------------
; RTL8139c +
;------------
[RTL8139P.ndi.NT]
AddReg          = RTL8139P.common.reg, RTL8139.reg, RTL8139P.W2K.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8139.CopyFiles

[RTL8139P.ndi.NT.Services]
AddService = rtl8139, 2, rtsnt.Service, RTL8139.EventLog

[RTL8139.CopyFiles]
R8139n5.sys,,,2

[RTL8139.CopyFiles98]
R8139n5.sys,,,2

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************

[rtl8139.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_10EC&DEV_8139"
HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\DuplexMode,             flag,   1,      30, 00, 00, 00
HKR, Ndi\Params\EarlyTxThreshold,       flag,   1,      20, 00, 00, 00
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00
HKR, NDI\Params\WakeUpFrame,            flag,   1,      30, 00, 00, 00

[RTL8139.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "Realtek RTL8139/810X Family Fast Ethernet NIC"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      r8139n5.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "RTL8139"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "rtl139.ndis5"

;;****************************************************************************
;; RTL8139 common parameters
;;****************************************************************************
;----------------
; RTL8139 Family
;----------------
[RTL8139.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "15"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,NDI\Params\TxInterFrameGap,flag,1,30,00,00,00
;HKR,Ndi\params\TxInterFrameGap,ParamDesc,0,"Tx IFG(10M/100M)"
;HKR,Ndi\params\TxInterFrameGap,type,0,enum
;HKR,Ndi\params\TxInterFrameGap,default,0,3
;HKR,Ndi\params\TxInterFrameGap\enum,0,0,"8.4us/840ns"
;HKR,Ndi\params\TxInterFrameGap\enum,1,0,"8.8us/880ns"
;HKR,Ndi\params\TxInterFrameGap\enum,2,0,"9.2us/920ns"
;HKR,Ndi\params\TxInterFrameGap\enum,3,0,"9.6us/960ns"

HKR,Ndi\params\RxBufLen,	   ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	   type,       0, "enum"
HKR,Ndi\params\RxBufLen,	   default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,	   "0",	       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "1",	       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "2",	       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "3",	       0, "64K bytes"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"
HKR, Ndi\params\WakeUpFrame,       default,    0, "1"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"

HKR, Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"
HKR, Ndi\params\RTPME,             default,    0, "0"
HKR, Ndi\params\RTPME,             type,       0, "enum"
HKR, Ndi\params\RTPME\enum,        "1",        0, "Enable"
HKR, Ndi\params\RTPME\enum,        "0",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

;------------
; RTL8139c +
;------------
[RTL8139P.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "15"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,"1",30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,"enum"
;HKR,Ndi\params\TxMaxDMABurst,default,0,"7"
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,"1",30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,"enum"
;HKR,Ndi\params\RxMaxDMABurst,default,0,"7"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,"enum"
;HKR,Ndi\params\EarlyRxThreshold,default,0,"2"
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,Ndi\Params\NumTcb, ParamDesc, 0, "Number of Tcb"
;HKR,Ndi\Params\NumTcb, Type,      0, "int"
;HKR,Ndi\Params\NumTcb, Default,   0, "48"
;HKR,Ndi\Params\NumTcb, Min,       0, "4"
;HKR,Ndi\Params\NumTcb, Max,       0, "63"
;HKR,Ndi\Params\NumTcb, Step,      0, "1"
;HKR,Ndi\Params\NumTcb, Base,      0, "10"

;HKR,Ndi\Params\NumRfd, ParamDesc, 0, "Number of Rfd"
;HKR,Ndi\Params\NumRfd, Type,      0, "int"
;HKR,Ndi\Params\NumRfd, Default,   0, "96"
;HKR,Ndi\Params\NumRfd, Min,       0, "4"
;HKR,Ndi\Params\NumRfd, Max,       0, "128"
;HKR,Ndi\Params\NumRfd, Step,      0, "1"
;HKR,Ndi\Params\NumRfd, Base,      0, "10"

;HKR,Ndi\Params\NumTxDesc, ParamDesc, 0, "Number of Tx Descriptor"
;HKR,Ndi\Params\NumTxDesc, Type,      0, "int"
;HKR,Ndi\Params\NumTxDesc, Default,   0, "63"
;HKR,Ndi\Params\NumTxDesc, Min,       0, "4"
;HKR,Ndi\Params\NumTxDesc, Max,       0, "63"
;HKR,Ndi\Params\NumTxDesc, Step,      0, "1"
;HKR,Ndi\Params\NumTxDesc, Base,      0, "10"


;HKR,Ndi\Params\NumRxDesc, ParamDesc, 0, "Number of Rx Descriptor"
;HKR,Ndi\Params\NumRxDesc, Type,      0, "int"
;HKR,Ndi\Params\NumRxDesc, Default,   0, "63"
;HKR,Ndi\Params\NumRxDesc, Min,       0, "4"
;HKR,Ndi\Params\NumRxDesc, Max,       0, "63"
;HKR,Ndi\Params\NumRxDesc, Step,      0, "1"
;HKR,Ndi\Params\NumRxDesc, Base,      0, "10"

HKR,Ndi\Params\NumCoalesce, ParamDesc, 0, "Number of Tx Coalesce Buffer"
HKR,Ndi\Params\NumCoalesce, Type,      0, "int"
HKR,Ndi\Params\NumCoalesce, Default,   0, "16"
HKR,Ndi\Params\NumCoalesce, Min,       0, "0"
HKR,Ndi\Params\NumCoalesce, Max,       0, "32"
HKR,Ndi\Params\NumCoalesce, Step,      0, "1"
HKR,Ndi\Params\NumCoalesce, Base,      0, "10"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"
HKR, Ndi\params\WakeUpFrame,       default,    0, "1"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

;HKR, Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"
;HKR, Ndi\params\RTPME,             default,    0, "0"
;HKR, Ndi\params\RTPME,             type,       0, "enum"
;HKR, Ndi\params\RTPME\enum,        "1",        0, "Enable"
;HKR, Ndi\params\RTPME\enum,        "0",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

;HKR, Ndi\params\CpuUtFlag,        ParamDesc,  0, "CPU Utilization Tuning"
;HKR, Ndi\params\CpuUtFlag,        default,    0, "3"
;HKR, Ndi\params\CpuUtFlag,        type,       0, "enum"
;HKR, Ndi\params\CpuUtFlag\enum,   "0",        0, "Disabled"
;HKR, Ndi\params\CpuUtFlag\enum,   "1",        0, "Transmit"
;HKR, Ndi\params\CpuUtFlag\enum,   "3",        0, "Transmit & Receive"

;HKR, Ndi\params\TxIFG,       ParamDesc,  0, "Tx IFG(10M/100M)"
;HKR, Ndi\params\TxIFG,       default,    0, "0"
;HKR, Ndi\params\TxIFG,       type,       0, "enum"
;HKR, Ndi\params\TxIFG\enum,  "0",        0, "Default Gap"
;HKR, Ndi\params\TxIFG\enum,  "1",        0, "0.8us/80ns"
;HKR, Ndi\params\TxIFG\enum,  "2",        0, "1.6us/160ns"
;HKR, Ndi\params\TxIFG\enum,  "3",        0, "2.4us/2400ns"
;HKR, Ndi\params\TxIFG\enum,  "4",        0, "3.2us/320ns"
;HKR, Ndi\params\TxIFG\enum,  "5",        0, "4.0us/400ns"
;HKR, Ndi\params\TxIFG\enum,  "6",        0, "4.8us/480ns"
;HKR, Ndi\params\TxIFG\enum,  "7",        0, "9.6us/960ns"

[RTL8139P.W2K.reg]
HKR, Ndi\params\Offload,             ParamDesc,  0, "Task Offload"
HKR, Ndi\params\Offload,             default,    0, "1"
HKR, Ndi\params\Offload,             type,       0, "enum"
HKR, Ndi\params\Offload\enum,        "0",        0, "All Disable"
HKR, Ndi\params\Offload\enum,        "1",        0, "Checksum"
HKR, Ndi\params\Offload\enum,        "2",        0, "Chksum & TCP_Segment"

HKR, Ndi\params\Support8021p,        ParamDesc,  0, "802.1Q/1p VLAN Tagging"
HKR, Ndi\params\Support8021p,        default,    0, "0"
HKR, Ndi\params\Support8021p,        type,       0, "enum"
HKR, Ndi\params\Support8021p\enum,   "0",        0, "Disable"
HKR, Ndi\params\Support8021p\enum,   "1",        0, "Enable"

;HKR,Ndi\Params\NumTcbHPQ,    ParamDesc, 0, "Number of High Priprity Tcb"
;HKR,Ndi\Params\NumTcbHPQ,    Type,      0, "int"
;HKR,Ndi\Params\NumTcbHPQ,    Default,   0, "48"
;HKR,Ndi\Params\NumTcbHPQ,    Min,       0, "4"
;HKR,Ndi\Params\NumTcbHPQ,    Max,       0, "63"
;HKR,Ndi\Params\NumTcbHPQ,    Step,      0, "1"
;HKR,Ndi\Params\NumTcbHPQ,    Base,      0, "10"

;HKR,Ndi\Params\NumTxDescHPQ, ParamDesc, 0, "Number of High Priority Tx Descriptor"
;HKR,Ndi\Params\NumTxDescHPQ, Type,      0, "int"
;HKR,Ndi\Params\NumTxDescHPQ, Default,   0, "63"
;HKR,Ndi\Params\NumTxDescHPQ, Min,       0, "4"
;HKR,Ndi\Params\NumTxDescHPQ, Max,       0, "63"
;HKR,Ndi\Params\NumTxDescHPQ, Step,      0, "1"
;HKR,Ndi\Params\NumTxDescHPQ, Base,      0, "10"


;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8139.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8139"

[rtsnt.Service]
DisplayName     = %RTL8139.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\R8139n5.SYS
LoadOrderGroup  = NDIS

[RTL8139.EventLog]
Addreg = RTL8139.AddEventLog.reg

[RTL8139.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTL8139.CopyFiles           = 12
RTL8139.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
r8139n5.sys  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek                   = "Realtek"

;;Source disk name
DISKNAME = "Realtek RTL8139/810X Family Fast Ethernet NIC Driver"

NetworkAddress            = "Network Address"
EarlyTxThreshold          = "Early Tx Threshold"
SpeedDuplexMode           = "Link Speed/Duplex Mode"
dmAutoMode                = "Auto Mode"
dm10HalfMode              = "10 Half Mode"
dm10FullMode              = "10 Full Mode"
dm100HalfMode             = "100 Half Mode"
dm100FullMode             = "100 Full Mode"

RTL8139.DeviceDesc        = "Realtek RTL8139/810X Family Fast Ethernet NIC"
RTL8139P.DeviceDesc       = "Realtek RTL8139 C+ Fast Ethernet NIC"

;;NT service name
RTL8139.Service.DispName = "Realtek RTL8139/810X Family Fast Etnernet NIC NT Driver"
