   Windows 98, Windows 98 SE, Windows2000, Windows ME

   Introduction:
   -------------
   This document describes the procedure to install Windows 98/98 SE
   Windows 2000 and Windows ME driver for Realtek RTL8139 PCI Fast
   Ethernet adapter.

   Location of Windows 98/98 SE Driver :   \win98\RTL8139.SYS
   Location of Windows 2000 Driver     :   \win2000\RTL8139.SYS
   Location of Windows ME Driver       :   \winme\RTL8139.SYS

   Installing driver for Win98/Win98 SE/Windows2000/Windows ME :
   -------------------------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Win98/Win98 SE/Windows2000/Windows ME, it will auto-detect
      your system configuration and find the adapter hardware.
      ( If Win98/Win98 SE/Windows2000/Windows ME does not prompt that it 
      detects the PCI Ethernet adapter,there must be something wrong with
      the RTL8139 PCI Fast Ethernet adapter or your system enviroment.)

      1. Ask you to select which driver you want to install, select "Driver
         from disk provided by hardware manufacturer".

      2. Insert the Realtek RTL8139 driver disk into drive A and specify
         the setup file pathname A:\WIN98 (for Windows 98/98 SE) or
                                 A:\WIN2000  (for Windows 2000)
                                 A:\Windows ME (for Windows ME)
                                 
      3. Win98/Win98 SE/Windows2000/Windows ME will appear some messages
         to insert Win98/Win98 SE/Windows2000/Windows ME system disk to
         complete setup step.

      4. Win98/Win98 SE/Windows2000/Windows ME will finish the other 
         installation procedure automatically, then you restart the system.

