   Windows 95 (Golden version), Win95A and OSR2

   Introduction:
   -------------
   This document describes the procedure to install  Windows 95 (Golden
   version), Win95A and OSR2 driver for Realtek RTL8139 PCI Fast Ethernet
   adapter.

   Location of Windows 95 and Win95A Driver:     \WIN95A\RTL8139.SYS
   Location of Windows 95 OSR2             :     \W95OSR2\RTL8139.SYS

   Installing driver procedure on Microsoft Windows 95 :
   -----------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Windows 95, it will auto-detect your system configuration
      and find the adapter hardware.  ( If Win95 does not  prompt that it
      detects the PCI Ethernet adapter,there must be something wrong with
      the RTL8139 PCI Fast Ethernet adapter or your system enviroment.)

      1. Ask you to select which driver you want to install, select "Driver
         from disk provided by hardware manufacturer".

      2. Insert the Realtek RTL8139 driver disk into drive A and specify
         the setup file pathname A:\WIN95A (for Windows 95 and Win95A) or
                                 A:\ (for Windows 95 OSR2) .

      3. Windows 95 will appear some messages to insert Windows 95 system
         disk to complete setup step.

      4. Windows 95  will  finish  the  other  installation  procedure
         automatically, then you restart the system.

