###############################################################################################
#
# Edit this file to give non-default values to FPF fuses
# using the FPF flash mirror. This file is used by FpfMirrorGenerateNvar.pl
# script. Each line in this file describes a fuse file in the following pattern:
#
# [ID]:[Value]
#
# ID 	 - Fuse file ID (see FUSE_FILE_XXX in FpfHeciMsgs.h)
# Value  - Desired value of fuse file in **hex** digits, must be byte-aligned (For single bit file, should be 00 or 01)
#
# For example, If this file contains the following line:
#
# FUSE_FILE_OEM_KEY_HASH_1:87c558E1FBBA60F7A87E58372D7CCC3BBB704DDB8E2144907C88FA1465A86FEA
#
# Then the Key_hash_1 file will be locked and will have the value:
#
#		 {0x87,0xc5,0x58,0xE1,0xFB,0xBA,0x60,0xF7,0xA8,0x7E,0x58,0x37,0x2D,0x7C,0xCC,0x3B,
#         0xBB,0x70,0x4D,0xDB,0x8E,0x21,0x44,0x90,0x7C,0x88,0xFA,0x14,0x65,0xA8,0x6F,0xEA} 
#	
# 
# Alt_bios_limit file is 16 bits wide; applicable values are up to 0x1FFF (13 bits effective).
# For the following line:
#
# FUSE_FILE_ALT_BIOS_LIMIT:1FFF
#
# The effective integer value will be: 0x1FFF
#  
###############################################################################################

#This Fuse bit is for enabling Verified Boot. Change value to "01" to enable Secure/verified boot
FUSE_FILE_SECURE_BOOT_EN:00

#This Fuse bit is for Disabling Intel(R) PTT. set value to '01' to permanently disable Intel(R) PTT (ftpm)
FUSE_FILE_TPM_DISABLE:00

#Hash of the public part of the OEM signing key obtained with the Flamingo tool
FUSE_FILE_OEM_KEY_HASH_1:0000000000000000000000000000000000000000000000000000000000000000

#The 13 Most Significant Bits of address of alternate copy of IBB within BIOS region
#Alt_bios_limit file is 16 bits wide; applicable values are up to 0x1FFF (13 bits effective).
FUSE_FILE_ALT_BIOS_LIMIT:0000

#This is the ID of the of the Key Manifest ('0' indicates no key manifest is required)
FUSE_FILE_KEY_MANIFEST_ID:00

