Step[01] - Flash BIOS and EC
	01-01.	Running Flash.nsh to flash bios and EC.

Step[02] - Flash Intel ME FW.
	02-01. Set secure boot to disable and modify BootOrder for boot to shell next boot up then press F4 to Save&Reset.
	02-02. Press "LeftCtrl" + "F1" key after power on,confirm to unlock ME when popup warning message,system will do coldreset and unlock ME region.
	02-03. boot to shell and run FlashME.nsh to update ME region.
	02-04. After flash complete,shutdown and remove AC power then re-plug in AC to fully do ME re-initialization.

